{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":38,"n_cols":13,"rows_kept":38,"merged":[[0,0,0,12],[1,0,1,12],[34,0,34,9],[35,0,35,9],[36,0,36,9],[37,0,37,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年7月电气备件采购项目                  项目编号：HG JY-G2024096"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,"A2246000390076",5601500006,"点火棒","SX-SHW-600","功率600W;电源220VAC","GB/T12011-2009","根",15,"炼钢厂部","2024-08-27"]
[2,"A2246000590001",6000201254,"真空断路器","ZN85-40.5 2500A/31.5kA","额定频率50Hz 额定电流 2500A 额定短路开断电流 31.5KA 额定峰值耐受电流80KA 操作顺序;分-0.3S-合分-180S-合分; 操作电压DC220V","GB/T21706-2008","台",1,"能源厂部","2024-08-27"]
[3,"A2246000590002",6000201255,"真空断路器","ZN85-40.5  1600A/31.5kA","额定频率50Hz 额定电流 1600A 额定短路开断电流 31.5KA 额定峰值耐受电流80KA 操作顺序;分-0.3S-合分-180S-合分; 操作电压DC220V","GB/T21706-2008","台",1,"能源厂部","2024-08-27"]
[4,"A2246000580002",6100100252,"微机消谐装置","CXDL-WXZ-N2","AC/DC220V;50-60HZ;环境温度-20-50℃；可消除谐振频率17HZ,25HZ,50HZ,150HZ","GB/T14285-2006","个",1,"能源厂部","2024-08-27"]
[5,"A2246000390059",6100200060,"隔离开关","SIWOG1(GL)-250/3J","Ue;380V;Ie;250A;50Hz;AC-23B","GB/T14048.3","台",1,"炼钢厂部","2024-08-27"]
[6,"A2246000390060",6100200061,"隔离开关","SIWOG1(GL)-400/3J","Ue;380V;Ie;400A;50Hz;AC-23B","GB/T14048.3","台",1,"炼钢厂部","2024-08-27"]
[7,"A2246000390061",6100200062,"隔离开关","SIWOG1(GL)-630/3J","Ue;380V;Ie;630A;50Hz;AC-23B","GB/T14048.3","台",1,"炼钢厂部","2024-08-27"]
[8,"A2246000390062",6100200063,"隔离开关","SIWOG1(GL)-1000/3J","Ue;380V;Ie;1000A;50Hz;AC-22A","GB/T14048.3","台",1,"炼钢厂部","2024-08-27"]
[9,"A2246000390063",6100200064,"隔离开关","SIWOG1(GL)-1250/3J","Ue;380V;Ie;1250A;50Hz;AC-22A","GB/T14048.3","台",1,"炼钢厂部","2024-08-27"]
[10,"A2246000460007",6100400395,"行车切电阻接触器","SEM-1J300","工作电源220/380VAC;额定电流300A;控制电压220/380V;中文液晶显示","QYQJ0301004-2019","个",2,"炼钢厂部","2024-08-12"]
[11,"A2246000820017",6200100103,"管坯液压站伺服泵变频器","YCT75","INPUT:3PH AC 380-480V 139.0A 50/60Hz;\nOUTPUT:3PH AC0-480V,150.0A0-300Hz75KN\nChangzhou YongchiTechnology Co..Ltd","GB/T12668.2-1989","台",1,"340热轧","2024-07-28"]
[12,"A1246000360109",6200200877,"750系列通信线","20-750-FCBL1-F8","750系列通用  0.56米","E0.967X","根",5,"219厂部","2024-09-26"]
[13,"A2246000390020",6200300120,"直流电源","JWAK-35S5D15S12NI","输入165-265VAC;输出电压12V/1A;±15V/0.5A;5V/0.5A","GB4943.1：2011","台",2,"炼钢厂部","2024-08-27"]
[14,"A1246000300003",6200300122,"箱式电阻炉炉膛","SX2-10-12NP-LT","三段式镍铬丝加热，炉膛尺寸318*242*415，最高温度1200℃，输入功率10KW","GB/T 9623","件",1,"检验检测中心","2024-08-27"]
[15,"A1246000360136",6300600089,"行车遥控装置","F23-BB 控制电压220V，带急停、钥匙开关，10按键（含起、停按钮）","2发一收，非晶振型，按键方向标注（起动、停止、上、下、左、右、前、后、1、2）","GB/T22084.2-2008","套",2,"219厂部","2024-08-27"]
[16,"A2246000390054",6400300252,"行程开关","ML441-11Y-T-2512-6","防护等级IP65;AC-15;Uimp4KV;Ui250V","IEC60947-5-1","个",5,"炼钢厂部","2024-08-27"]
[17,"A2246000390055",6400300253,"行程开关","MR441-11Y","防护等级IP65;AC-15;Uimp4KV;Ui250V","IEC60947-5-1","个",5,"炼钢厂部","2024-08-27"]
[18,"A2246000700268",6400400184,"旋转编码器","87XFW975","极对数1；励磁电压7W；励磁频率10kHz；变压比0.5±10%；允许最大转速800rpm","Q/DXJ 325-2019","台",2,"180热轧","2024-08-27"]
[19,"A2246000390050",6400600584,"激光测距仪","LMD2430-A","工作电压DC24V;电流最小值4.000mA;电流 最大值20.017mA","Q/3204BCK010-2013","台",1,"炼钢厂部","2024-08-27"]
[20,"A1246000310003",6400600612,"栏杆机红外对射","DS436i-chi,","工作电压：12V，警戒距离60米，射束距离650米。","GB/T27664.2-2010","对",2,"物流中心","2024-07-28"]
[21,"A1244000600011",6100500063,"时间继电器","ST3P A-F","AC220V 时间范围2小时","GB 10963.1","只",10,"89管加工热处理","2024-08-27"]
[22,"A1246000120019",6000300206,"电机保护器","HYCLD-F-3","环境温度：-30一+70，额定工作电压：110v、220v、380Ⅴ充许偏差±20%，可现场设定额定电流，380v一660vAC三相异步电动机、馈线电容保护，PS485通迅接口，防护lP67",null,"个",3,"物流中心","2024-08-27"]
[23,"A2244000310046",6600300196,"阀门回讯器","TXP-M20GNPM","2xSPDT无源干接点;触点容量10A;250VAC;隔爆型Ex d II C T4;IP67防护等级","GB/T12237","个",6,"炼钢厂部","2024-08-27"]
[24,"A2244000310088",6100900078,"动力箱（壳体）","6.14.100.4；尺寸：宽350*深260*高280；","采用2mm钢板制作；下进线(下方开孔）；配接地柱；表面刷漆，冰灰GY09","图纸审核","个",10,"炼钢厂部","2024-08-27"]
[25,"A2244000310089",6100900005,"不修钢辊道开关箱","530*500*400 非标","非标 不锈钢制作",null,"台",10,"炼钢厂部","2024-08-27"]
[26,"A2244000430071",6100100097,"整流控制柜变压器","ZSG-30KVA/170+190","GB/T18494.1-2001 30KVA 输入380V 输出170+190V","JB4315-1986","台",1,"340热轧","2024-08-27"]
[27,"A2245000440054",6300500280,"不间断电源","3C10KS(6G)","容量10KVA/9Kw;电池输入192VDC;旁路输入220VAC;50Hz;63A;输出220VAC;50Hz;5.5A","GB/T9813-2000","台",1,"炼钢厂部","2024-08-27"]
[28,"A2246000220047",6100900180,"变频控制柜","柜体尺寸：长800*宽800*高2200","柜内包含：LC1D475交流接触器，NSX630N断路器，6SL3310-1TE35-0AA3变频器，DBU-4220B制动单元，6SL3040-0LA00-0AA1控制单元","德国IEC947","台",1,"180热轧","2024-08-27"]
[29,"A1245000450031",6400600183,"限位开关","LX44-20 AC380V 20A","GB/T14048,电动葫芦限位开关","GB/T14048","只",5,"89管加工热处理","2024-08-27"]
[30,"A1246000120007",4100800036,"稳压电源","WY-1285","AC220V/DC12V GB14048.4-93","GB14048.4-93","台",3,"物流中心","2024-08-27"]
[31,"A2245000440062",4000100154,"指示灯","AD16-22B","220VDC （红）","EN60947-511EC337","只",20,"炼钢厂部","2024-08-27"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年7月电气备件采购项目        项目编号：HG JY-G2024096"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]