{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一、开标一览表","index":0,"n_rows":65,"n_cols":11,"rows_kept":65,"merged":[[0,0,0,10],[1,0,1,10],[62,0,62,10],[63,0,63,10],[64,0,64,10]],"flags":["formulas_cached_only"]}
["开  标  一  览  表"]
["项目名称：2024年8月-2025年8月五金日杂年标采购项目                               项目编号：HG JY-G2024095"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,4000700090,"一吨包装袋","装载量1吨",null,"件",3000,"以订单为准",null,null,"需求量以订单为准"]
[2,4000200040,"阀控密封铝酸电池","GFM300 CHAMPION","2V  300AH","只",100,"以订单为准",null,null,"需求量以订单为准"]
[3,4600100060,"防尘口罩","9502V+KN95","折叠式带阀","只",80000,"以订单为准",null,null,"需求量以订单为准"]
[4,3163100002,"高温喷号涂料","JR-100",null,"Kg",2000,"以订单为准",null,null,"需求量以订单为准"]
[5,8700800058,"RIHON利合牌微晶弹性抛光轮","SC80-300mm*50mm*32mm","材料硬度14P、抛光轮颜色：蓝色；原材料：微晶刚玉。性能：切削力强、粉尘少","个",200,"以订单为准",null,null,"需求量以订单为准"]
[6,4201700099,"纤维抛光轮","外径*厚度*中心孔：300mm*50mm*33mm","材料硬度等级：14P","块",2500,"以订单为准",null,null,"需求量以订单为准"]
[7,4600100059,"防尘口罩","9501V+KN95","折叠式带阀","只",80000,"以订单为准",null,null,"需求量以订单为准"]
[8,4600100025,"马头牌肥皂","200克",null,"块",50000,"以订单为准",null,null,"需求量以订单为准"]
[9,3301000055,"切削液","Master马思特 TRIM  SC310，每桶量：204L","水溶液推荐使用浓度： 3.0% - 10.0%","桶",10,"以订单为准",null,null,"需求量以订单为准"]
[10,4600100097,"炼铁全棉阻燃服","340g宝兰全棉阻燃面料","成分:纱支21S/2x21S/3  密度88 根/inch*32 根/inch,","套",500,"以订单为准",null,null,"需求量以订单为准"]
[11,4600100017,"防护面屏安全帽支架","BD173B",null,"个",2850,"以订单为准",null,null,"需求量以订单为准"]
[12,4600100098,"防护面屏","SE-173A-Plus",null,"块",2500,"以订单为准",null,null,"需求量以订单为准"]
[13,4300600061,"应力环盒子进气出气口接头","T-400-1-4","PTFE材质，硫化氢腐蚀；包含公扣母扣，连接1/4英寸气管，一端是1/4NPT外螺纹连接，另外一端是1/4英寸卡套连接","套",200,"以订单为准",null,null,"需求量以订单为准"]
[14,5300800023,"送样专用三轮电动车","车身尺寸：3130*1110*1380，箱体尺寸：1600*1100*260","技术参数：功率1000w,电瓶45A;车速≤25km/h;带驾驶室；把式","台",10,"以订单为准",null,null,"需求量以订单为准"]
[15,3400100067,"过滤器填充料；无烟煤滤料","直径2~4mm","密度为1.57g/cm3。盐酸可溶率不应大于0.81%；","吨",60,"以订单为准",null,null,"需求量以订单为准"]
[16,4600100041,"耳塞1110子弹型","（两只要有线连接）",null,"付",27000,"以订单为准",null,null,"需求量以订单为准"]
[17,4600100010,"带嘴型防尘口罩","（3M3200型面具及3700型承接座）",null,"套",1600,"以订单为准",null,null,"需求量以订单为准"]
[18,7501100510,"卡套","T-400-SET","材质：特氟龙，与1/4英寸硫化氢气管相接的前后卡套","套",800,"以订单为准",null,null,"需求量以订单为准"]
[19,3301000009,"亚硝酸钠","（工业用)",null,"吨",7,"以订单为准",null,null,"需求量以订单为准"]
[20,3301000026,"锯床专用切削液","HJ-Y01；5Kg/桶",null,"桶",1000,"以订单为准",null,null,"需求量以订单为准"]
[21,4201200034,"冲击试验机缺口拉刀","QCS-Y-2T;V/U型;W18Cr4V;HRC65-70;54齿;GB/T229",null,"个",8,"以订单为准",null,null,"需求量以订单为准"]
[22,6700400213,"英思特朗150吨拉伸机平板夹具","英思特朗1500KN万能试验机;专用拉伸夹具平钳口;5-25mm,一套共上下左右四块","适用于5-25mm，专用拉伸夹具平钳口","套",4,"以订单为准",null,null,"需求量以订单为准"]
[23,6600200727,"HXFQ-6S型焦炭反应性及反应后强度测定仪焦炭反应器","HXFQ-6S-FYQ","反应器耐高温合金钢，材质为GH3044,内径80mm±1mm,反应管壁厚不小于1.5mm，拖料筛片直径78±1mm，其上均匀钻3mm圆孔，孔间距5mm，筛片厚度1.5mm","套",7,"以订单为准",null,null,"需求量以订单为准"]
[24,4201700064,"园锥磨头","直径20*30",null,"只",32500,"以订单为准",null,null,"需求量以订单为准"]
[25,6700400155,"硫化氢实验堵头","非标，配M10试样",null,"只",210,"以订单为准",null,null,"需求量以订单为准"]
[26,4200700034,"酷刚玉砂轮片","230*6*22",null,"片",500,"以订单为准",null,null,"需求量以订单为准"]
[27,4300500029,"同步齿形带","BD114MGT-2520 USA278*26",null,"根",4,"以订单为准",null,null,"需求量以订单为准"]
[28,3400100062,"过滤器填充料；卵石","直径4mm~8mm","\"SiO2含量≥98% ；盐酸可溶率≤3.5% ；密度2.66g/cm3；堆密度1.85g/cm3\n　　\"","吨",30,"以订单为准",null,null,"需求量以订单为准"]
[29,3400100063,"过滤器填充料；卵石","直径2mm~4mm","\"SiO2含量≥98% ；盐酸可溶率≤3.5% ；密度2.66g/cm3；堆密度1.85g/cm3\n　　\"","吨",30,"以订单为准",null,null,"需求量以订单为准"]
[30,4000200059,"黄腊玻璃丝管直径","直径20mm",null,"根",1500,"以订单为准",null,null,"需求量以订单为准"]
[31,4000200061,"黄腊玻璃丝管直径","直径35mm",null,"根",1000,"以订单为准",null,null,"需求量以订单为准"]
[32,4100900001,"不锈钢电焊条A132","直径3.2 E308-16",null,"Kg",400,"以订单为准",null,null,"需求量以订单为准"]
[33,4100900002,"不锈钢电焊条A132","直径4 E308-16",null,"Kg",400,"以订单为准",null,null,"需求量以订单为准"]
[34,4000400039,"平面密封胶","515 300g/支",null,"支",150,"以订单为准",null,null,"需求量以订单为准"]
[35,4000400078,"高效清洗剂","755；400ml/瓶","400ml/瓶","瓶",200,"以订单为准",null,null,"需求量以订单为准"]
[36,4000400174,"无尘工业擦拭纸","单张尺寸25*38cm","用于擦拭油污、液体;擦拭、清洁密封胶;500张/卷","卷",150,"以订单为准",null,null,"需求量以订单为准"]
[37,4000400182,"油漆笔","G-0971","线幅：1mm-3mm，防水防油；颜色包括白色，黑色，红色等","支",1000,"以订单为准",null,null,"需求量以订单为准"]
[38,4100900048,"修磨用钹形砂轮","BX A24QBF 125*6.0*22.2","XK06-011-00948 MAX.80m/s，MAX.R.P.M12200  红象","片",20000,"以订单为准",null,null,"需求量以订单为准"]
[39,4200200009,"电动扳手","BHTW-1000",null,"台",5,"以订单为准",null,null,"需求量以订单为准"]
[40,4200200154,"充电式电动扳手","18VDTW1001.0-2200/min（带电池，带充电器）","能力：M12-M30（1/2''-1-1/4''); 高强度螺栓M10-M24（3/8''-1''); 方形传动螺杆12.7mm(1/2'')  冲击数（ipm) 高/中/低0-2,200/0-2,000/0-1,800  回转数（rpm）高/中/低0-1,800/0-1,000/0-900  最大扭矩：1,000N.m(740ft.lbs)","台",8,"以订单为准",null,null,"需求量以订单为准"]
[41,5700100054,"圆弧齿同步齿形带","1568-14M-37（带宽）","GB11616-1989，进口材质","根",150,"以订单为准",null,null,"需求量以订单为准"]
[42,4300500030,"同步齿形带","HTD1890-14M",null,"根",150,"以订单为准",null,null,"需求量以订单为准"]
[43,4200700030,"角向磨光机","SIM-SD03-150A",null,"台",100,"以订单为准",null,null,"需求量以订单为准"]
[44,4200700066,"充电式砂轮机","RG2011","18V","台",8,"以订单为准",null,null,"需求量以订单为准"]
[45,4200800055,"手提式工具包","350x250x270mm 81008B",null,"把",40,"以订单为准",null,null,"需求量以订单为准"]
[46,4200900107,"可赛新1750松动剂","可赛新1750松动剂,350g/瓶",null,"个",80,"以订单为准",null,null,"需求量以订单为准"]
[47,4201700010,"对讲机","LT-3268 TIA/EIA-603","TIA/EIA-603","台",300,"以订单为准",null,null,"需求量以订单为准"]
[48,4200800012,"对讲机","GM360","配220V转换器","台",20,"以订单为准",null,null,"需求量以订单为准"]
[49,6400500234,"超声波探伤仪","HS600","HS600附合格证 附性能测试报告","台",2,"以订单为准",null,null,"需求量以订单为准"]
[50,4201700011,"附柄砂布轮.","附柄砂布轮80#",null,"个",5000,"以订单为准",null,null,"需求量以订单为准"]
[51,4400400045,"不锈钢切割用铁粉","25Kg/包;包装材料;PE-Foil","粒度(测试标准 DNI ISO 4497)：>160μm up to 2%， >100μm up to 35%；>63μm 20 up to 45%，<63μm 30 up to 60%；                           流量(测试标准 DNI ISO 4490)： 27s/50g。","Kg",6000,"以订单为准",null,null,"需求量以订单为准"]
[52,6400500127,"探伤机 漏磁纵向探头架","6.085-795-02 MIL-STD-1344A","附合格证 附性能测试报告","件",7,"以订单为准",null,null,"需求量以订单为准"]
[53,7102900055,"生料带","20m",null,"卷",1000,"以订单为准",null,null,"需求量以订单为准"]
[54,4201700135,"无磁无线对讲机","G-39","外形尺寸119*51*32;重量210g;信道16;频率范围400~470MHz;工作电压7.4V;电池容量3800mAh(标配);功率10W;待机时间135小时;发射电流<1.5A频率稳定性","台",200,"以订单为准",null,null,"需求量以订单为准"]
[55,4000700035,"水洗混纺无尘石棉编绳","*","直径20mm；","Kg",3600,"以订单为准",null,null,"需求量以订单为准"]
[56,4600100026,"毛巾","22864-2009",null,"条",5000,"以订单为准",null,null,"需求量以订单为准"]
[57,4600100086,"高隔热护腿","ABL-X032  45cm","常规款;材质芳纶镀铝;辐射热1000度","付",300,"以订单为准",null,null,"需求量以订单为准"]
[58,4600100088,"高隔热阻燃袖套","ABL-S1012 55cm","常规款;材质芳纶镀铝;辐射热1000度","双",300,"以订单为准",null,null,"需求量以订单为准"]
[59,4600100089,"高隔热阻燃围裙","ABL-V022 96cm","常规款;材质芳纶镀铝;辐射热1000度","块",20,"以订单为准",null,null,"需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年8月-2025年8月五金日杂年标采购项目                               项目编号：HG JY-G2024095"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]