{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":35,"n_cols":13,"rows_kept":35,"merged":[[0,0,0,12],[1,0,1,12],[31,0,31,12],[32,0,32,12],[33,0,33,12],[34,0,34,12]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年8月电动机采购项目                    项目编号：HG JY-G2024116"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"A2244000310017","6000201225","三相异步电动机","MS6324","额定功率0.2Kw;额定电压380V;额定电流0.72A;防护等级IP55;绝缘等级F级;安装方式B14;额定转速1350r/min;Y形接法，S3工作制","台","2","2024-10-30","炼钢厂部"]
[2,"A2244000310140","6000200295","绕线式转子电机","YZR160L-6H 11Kw 双轴","JB/T10105-1999 中心高度160 11KW 380V 6极 940r/min绝缘等级H 双轴输出","台","2","2024-10-30","炼钢厂部"]
[3,"A2246000390014","6000201204","高效率三相异步电动机","YE4-100L2-4;3KW；带小齿轮","额定电压 380V; 额定电流 6.5A; 额定转速 1430r/min ;绝缘等级F; 防护等级IP55 ; 安装方式B5 ;接线方式 Y;功率因素0.82;50HZ;出厂编号16201","台","1","2024-10-30","炼钢厂部"]
[4,"A2246000390032","6000201196","变频调速三相异步电动机","BPY-225M-6","额定功率30Kw;额定电压380V;额定电流61.6A;防护等级IP55;绝缘等级H级;频率50HZ;额定转速980r/min;安装方式B3;Y形接法","台","1","2024-10-30","炼钢厂部"]
[5,"A2246000390033","6000201199","变频调速三相异步电动机","YGP132M1-4E","额定功率3Kw;额定电压380V;额定电流6.4A;防护等级IP55;绝缘等级H级;频率50HZ;额定转速1460r/min;安装方式B5;Y形接法;S1工作制","台","5","2024-10-30","炼钢厂部"]
[6,"A2246000390034","6000201200","变频调速三相异步电动机","SME000840-21","额定功率90Kw;额定电压380V;额定电流162A;防护等级IP54;绝缘等级H级;频率50HZ;额定转速1475r/min;安装方式B3;Y形接法;S1工作制","台","1","2024-10-30","炼钢厂部"]
[7,"A2246000390035","6000201201","变频调速三相异步电动机","SME000840-76","额定功率55Kw;额定电压380V;额定电流105A;防护等级IP54;绝缘等级H级;频率50HZ;额定转速1475r/min;安装方式B3;Y形接法;S1工作制","台","1","2024-10-30","炼钢厂部"]
[8,"A2246000390037","6000201195","三相异步电动机","DM80M2-4-E","额定功率0.75Kw;额定电压380V;额定电流2.1A;防护等级IP55;绝缘等级F级;频率50HZ;额定转速1430rpm;安装方式B5;Y形接法","台","1","2024-10-30","炼钢厂部"]
[9,"A2246000390038","6000201197","三相异步电动机","SME000838-37","额定功率5.5Kw;额定电压380V;额定电流12.5A;防护等级IP54;绝缘等级H级;频率50HZ;额定转速933r/min;安装方式B3;Y形接法;S3工作制","台","1","2024-10-30","炼钢厂部"]
[10,"A2246000660036","6000201263","高效率三相异步电动机","YE3-80M1-4","额定电压 380V;功率0.55KW，额定电流 1.4A;额定转速 1430r/min;绝缘等级F;防护等级IP55;功率因毒0.75;50HZ","台","2","2024-10-30","340热轧"]
[11,"A2246000700219","6000200677","变频调速三相异步电动机","YVF2-90S-4;1.1Kw","额定电压380V;额定电流2.7A;额定转速1400r/min;绝缘等级F; 防护等级IP55; 接线方式:Y形","台","1","2024-10-30","180热轧"]
[12,"A2246000700269","6000200650","异步交流电动机","Y112M-4;4Kw","380V;绝缘等级F级;IP44;B5;△型接线方式;8.8A;1440r/min;电机尾端不带风叶与风罩;尾端轴不伸出尾端盖;出轴端钻孔攻丝φ10mm*25mm;前端法兰盘四个孔要带丝φ16mm","台","4","2024-10-30","180热轧"]
[13,"A2246000820013","6000201061","轧钢辊道电动机","YE3-112M-4G","配DSZR87-67,带小齿轮，功率：3KW;6.5A;额定转速:1405rpm;防护等级:IP55;频率:50HZ;安装方式:B5;出厂编号：1100049515/2-005;厂家:宁波东力","台","2","2024-10-30","340热轧"]
[14,"A2246000820018","6000201256","管坯液压站伺服泵电机","YC2571-F15R1P4","Un（V）380；In(A)140.6;FN(Hz)100；Pn(KW)70.7;Tn（N.m)450;Nn(rpm)1500;EFE96.3%,IP54 3PHAC,常州勇驰科技有限公司","台","1","2024-10-30","340热轧"]
[15,"A2247000270208","6000200028","变频电动机","YVP200L2-6 22Kw","AC380V F级 IP54 IM B3 接线 △型 接线盒位置 R(右) 43.8A 定额S1 额定转矩219.1N.m 恒转矩3-50Hz恒功率50-100Hz 冷却方式IC 416 标准编号JB/T7118-2014","台","1","2024-10-30","炼铁厂部"]
[16,"A2247000270213","6000200834","异步交流电动机","YEZ132S-6;4Kw","电流11A，转速930R/min 电压380V IP44 B5","台","1","2024-10-30","炼铁厂部"]
[17,"A2247000270214","6000200829","异步交流电动机","YEZ112S-4;3Kw","电流7.6A，转速1380R/min 电压380V IP44 B5","台","1","2024-10-30","炼铁厂部"]
[18,"A2247000270215","6000200830","异步交流电动机","YEZ112L-4;4.5Kw","电流10.5A，转速1380R/min 电压380V 50HZ IP44 B5","台","1","2024-10-30","炼铁厂部"]
[19,"A2247000270220","5300600046","电动葫芦 电机","ZDYE-31-4 3Kw",null,"台","1","2024-10-30","炼铁厂部"]
[20,"A2247000440013","6000200699","变频三相异步电动机","YSP315L-4","B3 185Kw 336A;;恒功率范围50－67HZ IP54 F级 接法 三角型","台","1","2024-10-30","炼钢厂部"]
[21,"A2247000440058","6000201262","起重及冶金用变频调速三相异步电动机","YZP250M1-8","功率30Kw;额定电压380V;额定电流63A;转速735r/min;绝缘等级H级;防护等级IP54;三角形接法;安装方式B3;S3工作制","台","1","2024-10-30","炼钢厂部"]
[22,"A2247000780086","6000201257","三相异步电动机","YE4-112M-4，配77-183","配DSZR77-183带小齿轮，功率：4KW;8.8A;额定转速:1434rpm;防护等级:IP55;频率:50HZ;出厂编号：1100051544/1-004;厂家:宁波东力","台","3","2024-10-30","340热轧"]
[23,"A2247000780087","6000201258","三相异步电动机","DMS0M2-4","额定功率：0.75KW;额定电压:380V;额定电流:21A;防护等级:IP55;频率:50HZ;额定转速:1414rpm;出厂编号1100043635/3-003;厂家:宁波东力","台","1","2024-10-30","340热轧"]
[24,"A2247000790202","6000201230","三相异步电动机","3-Mot./N\"/M 181757/0061 HIE1_K21R 160M 4 TWS HW","功率11KW;额定电压：400/690Δ/Y；额定电流21.5/12.5A;额度转速1455r/min;功率因数0.84；额定电压：380..420Δ；额定电流22.5..21.5A;额度转速1450..1460r/min;50HZ;功率因数0.81;防护等级：IP55；安装方式：B35;Rt.-30..+45℃ ;VEM","台","1","2024-10-30","180热轧"]
[25,"A2247000790212","6000201269","变频电动机","YP200L-4-L -M4-30Kw","带小齿轮，H级，额定电压380V;额定电流60.6A;额定转速 1480r/min;绝缘等级 H级; 防护等级 IP55 ;安装方式M4 ;△型接线方式; 出厂编号72528-4,用于DLK07-105;小齿轮安装方式采用止动垫圈加锁紧螺母方式","台","2","2024-10-30","180热轧"]
[26,"A2247000790215","6000201252","异步交流电动机","YTSZ250M-6","380V，45KW，85A，中心高250M，6级电机，绝缘等级H级，防护等级：IP55，传动方式：皮带传动，B35安装方式，电机轴45#钢调质，同轴风机","台","1","2024-10-30","180热轧"]
[27,"A1247000540034","6000201266","异步交流电动机","YE4  100L2-4  3KW B5","标准YE4系列电动机；额定电压交流380V；功率3kw；安装方式：B5（立式）；防护等级：IP55","台","2","2024-10-30","219厂部"]
[]
["注：1、投标报价含税，税率13% ；                                                                                                               \n 2、生产厂家要求全称填写准确无误 ；                                                                                                              \n 3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年8月电动机采购项目                    项目编号：HG JY-G2024116"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]