{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":13,"n_cols":13,"rows_kept":13,"merged":[[0,0,0,12],[1,0,1,12],[9,0,9,12],[10,0,10,12],[11,0,11,12],[12,0,12,12]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年8月仪器仪表采购项目                      项目编号：HG JY-G2024117"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"A2246000160215","6600201006","智能热像仪","BOETRNIK 525-L3","工作温度：-20℃～50℃；工作电源：12-24VDC；热像探测器像素：384×288像素；温度灵敏度： 0.05℃；空间分辨率：1.13毫弧度；具有2in1巡检和远测功能；标配镜头25°×19°；具有手动和自动对焦功能，1~8倍连续数码变焦；测温范围：-20℃~+2000℃，内置特征软件功能","台","3","2024-10-30","炼铁厂部"]
[2,"A2247000440041","6600201005","质量流量控制器","SLA5853S2GAB2C2A1","介质Ar;电源13.5-27VDC;4-20mA输出;量程0-600 SLPM;pro conn：1/2-in FNPT","台","1","2024-10-30","炼钢厂部"]
[3,"A2245000490001","6600200809","光谱分析仪;循环泵","订货号;75050027","LAB;PJ10247-023;0.07Kw;230V/0.55A;50-60Hz","台","1","2024-10-30","炼钢厂部"]
[4,"A2245000490002","6600200130","光谱分析仪 点火板","IGNITION SOURCE for SOURCE3000",null,"块","1","2024-10-30","炼钢厂部"]
[5,"A2245000490003","6600200807","光谱分析仪;光源","订货号;76020008","SOURCE3000","只","1","2024-10-30","炼钢厂部"]
[]
["注：1、投标报价含税，税率13% ；                                                                                                                2、生产厂家要求全称填写准确无误 ；                                                                                                               3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年8月仪器仪表采购项目                      项目编号：HG JY-G2024117"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]