{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":35,"n_cols":14,"rows_kept":35,"merged":[[0,0,0,12],[1,0,1,12],[31,0,31,9],[32,0,32,9],[33,0,33,9],[34,0,34,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年9月电气备件采购项目                  项目编号：HG JY-G2024121"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2247000160017",6100300112,"断路器","QMB1-63型 1P 32A",null,"IEC60947-2","只",5,"能源厂部","2024-10-11"]
[2,"A2247000270185",6400400074,"增量编码器","E6B2-CWZ6C CE","外 ?径: 40MM：轴 径: 6MM：输出方式: （增量式）：工作电压: DC5-24V：防护等级：IP50",null,"只",2,"炼铁厂部","2024-11-10"]
[3,"A2247000790183",4000200031,"电源","S-100-24","24V 4.5A","GB/T 15184-1994","只",5,"180热轧","2024-10-11"]
[4,"A2247000790197",6100100068,"联络组件","QB3-6 810233",null,"GB 17196-1997","片",500,"180热轧","2024-10-11"]
[5,"A1247000540038",6400400074,"增量编码器","E6B2-CWZ6C CE","外 ?径: 40MM：轴 径: 6MM：输出方式: （增量式）：工作电压: DC5-24V：防护等级：IP50",null,"只",2,"219厂部","2024-11-10"]
[6,"A1245000450033",6100400039,"交流接触器","CJ12-250/3","380V 灭弧罩为工程塑料","GB/T14048","只",5,"89管加工热处理","2024-10-11"]
[7,"A223C000540236",4000200371,"AC36V工业插头","插头;CEE-012 ；电压等级36VAC，",null,"GBT 11918-2014","个",20,"炼钢厂部","2024-10-11"]
[8,"A2245000440062",4000100154,"指示灯","AD16-22B","220VDC （红）","EN60947-511EC337","只",20,"炼钢厂部","2024-10-11"]
[9,"A1246000310003",6400600612,"栏杆机红外对射","DS436i-chi,","工作电压：12V，警戒距离60米，射束距离650米。","GB/T27664.2-2010","对",2,"物流中心","2024-10-11"]
[10,"A2245000180192",4000200371,"AC36V工业插头","插头;CEE-012 ；电压等级36VAC，",null,"GBT 11918-2014","个",30,"炼铁厂部","2024-06-27"]
[11,"A2247000160014",6100200023,"万能转换开关","LW12-16/40083/1",null,null,"个",5,"能源厂部","2024-09-26"]
[12,"A2248000440005",6200200990,"数字式（可控硅换向）调压调速装置","THYROMAT 10BCCH 350A 380BSZ-A","供电电压380V;3相50Hz;控制电压220V;单相50Hz;额定电流350A;电机定子电流250A-318A;起升机构应用","GB/T3235-1999","台",1,"炼钢厂部","2024-10-27"]
[13,"A2248000450020",6100100255,"出线电抗器","MC0-90/1","额定电流90A;电感值141μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[14,"A2248000450021",6100100256,"出线电抗器","MC0-240/1","额定电流240A;电感值53μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[15,"A2248000450022",6100100257,"出线电抗器","MC0-24/1","额定电流23.7A;电感值540μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[16,"A2248000450023",6100100258,"进线电抗器","MCI-20/1","额定电流20A;电感值704μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[17,"A2248000450024",6100100259,"出线电抗器","MC0-48/1","额定电流48A;电感值260μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[18,"A2248000450025",6100100260,"进线电抗器","MCI-35/1","额定电流35A;电感值402μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[19,"A2248000450026",6100100261,"出线电抗器","MC0-52/1","额定电流52A;电感值244μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[20,"A2248000450027",6100100262,"出线电抗器","MC0-70/1","额定电流70A;电感值181μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-10-27"]
[21,"A2248000470200",7101500113,"阀门电动装置","XZA20-18.T","输出转速18r/min;输出扭矩200N.m;防护等级:IP67","GB/T24923-2010","台",2,"炼钢厂部","2024-10-27"]
[22,"A2248000470201",7101500114,"电动执行器","STQ25B无源型","电源AC220V;力矩250NM;电机功率40W;接线标准M20*1.5;防护等级:IP67;开关时间45S;连接尺寸90(22.3)","GB/T24923-2010","台",2,"炼钢厂部","2024-10-27"]
[23,"A2248000620133",6100900181,"周轧机操作台","TG720101","1200*800*800(W*D*H),包含柜体、背板、台面开关、按钮、指示灯、标牌、模块、断路器、端子排，柜内无需接线","审核图纸","台",1,"720厂部","2024-10-11"]
[24,"A2248000620134",6100900182,"芯棒循环操作台","TG720102","1200*800*800（W*D*H)包含柜体、背板、台面按钮、开关、指示灯、标牌、模块、断路器、端子排，柜内接线见图纸","审核图纸","台",1,"720厂部","2024-10-11"]
[25,"A1247000510035",6200200725,"操作面板","20-HIM-A6","PowerFlex 753系列变频器操作面板","E0.967X","个",2,"89管加工热处理","2024-10-26"]
[26,"A1248000450022",6100900193,"操作台","89厂精整2#线喷标操作台1000*610*810","活动面板、活动正门，内装隔板一边装端子排，一边装工控机，后面开孔做鼠标、键盘电源等出线口。304不锈钢面板，上面按图开孔以便安装施耐德按钮，转换开关，急停按钮，称重仪，并装好标识牌。","审核图纸","个",1,"89管加工热处理","2024-10-11"]
[27,"A1248000480142",6300500287,"语音提示器","BY-F800","RS485+RTU版 9-26V 尺寸 100*100*43.5 自带5W喇叭 通过USB可更换语音，可外接喇叭和警灯 可端子控制和网络控制，8M内存","GB14048.5-2008","台",10,"219厂部","2024-10-11"]
[28,null,null,"高频电源","EHC-II 1.2A/80KV",null,"详见技术规格书","套",1,"炼铁烧结主厂房等封闭项目HG202418","2024-10-11"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年9月电气备件采购项目         项目编号：HG JY-G2024121"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]