{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":16,"n_cols":14,"rows_kept":16,"merged":[[0,0,0,9],[1,0,1,13],[12,0,12,9],[13,0,13,9],[14,0,14,9],[15,0,15,9]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年10月机械备件采购项目Ⅱ               项目编号：HG JY-G2024139"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2248000830015",6600300033,"煤气调节阀","E75B/WSO-11.15-AP/PSDH","阀门口径 DN150 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 额定CV值：1350 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ 执行机构型号 S93气动角行程，高温型≤120℃ 气源压力0.4~0.6Mpa 阀门定位器S67Y（高温型≤120℃），","只",1,"GB/T4213-1992","180热轧","2024-12-27"]
[2,"A224A000070020",7502000190,"高压泵;铜螺母","0540201.01.03;","ZCuAl10Fe3;    804Kg","件",1,"JB/T 5000","340管加工热处理","2024-12-27"]
[3,"A2248000800053",7101600281,"高温烟气调节阀","LSQF-1W-G","DN1700;输入信号4-20mADC，输出4-20mADC;阀杆，阀体不锈钢，工作温度0-450℃；质保2年，宗曼（上海）阀门制造有限公司","台",1,"GB/T4213-2008","180管加工热处理","2024-12-27"]
[4,"A1249000090009",4300500129,"废橡胶皮带","成捆","不得夹杂碎皮带及钢丝皮带","吨",30,"GB7984-2001-T","物流中心","2024-12-27"]
[5,"A2249000540003",7001500013,"Y型真空泵机身总成","WLW-2400B","尺寸：1920mm×1080mm×1900mm；中心距1100mm；材质：铸铁HT200；含曲轴、连杆、十字头、大小头轴瓦、活塞杆等全套，具体见技术协议","套",1,"Q/SOEU17-2007","能源厂部","2024-12-27"]
[6,"A2249000750021",4000500074,"方孔手筛","1000*700*150，方孔5mm",null,"台",1,"GB/T 12620-2008","高辅工段","2024-12-27"]
[7,"A2249000750022",4000500075,"方孔手筛","1000*700*150，方孔8mm",null,"台",1,"GB/T 12620-2008","高辅工段","2024-12-27"]
[8,"A2249000750023",4000500076,"方孔手筛","1000*700*150，方孔10mm",null,"台",1,"GB/T 12620-2008","高辅工段","2024-12-27"]
[9,"A2249000350012",6600300146,"雾化调节阀","OKV2107057-6","定位器 TYPE:RAD-RH/POS1 SIZE:400 BENCH SET:0-33 TRAVEL 90DegC PRESS UNITS: PSI  阀体 TYPE:1001 SIZE:3 PORT SIZE:3 RATING:CL150RF PLUG CF3M/CR PL STEM: S20910 BODY:WCC SEAT:S21800","台",1,"ASME","炼钢厂部","2024-12-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年10月机械备件采购项目Ⅱ        项目编号：HG JY-G2024139"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}