{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":29,"n_cols":13,"rows_kept":29,"merged":[[0,0,0,12],[1,0,1,12],[25,0,25,12],[26,0,26,12],[27,0,27,12],[28,0,28,12]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年11月电动机招标采购项目                      项目编号：HG JY-G2024141"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"A2244000310017","6000201225","三相异步电动机","MS6324","额定功率0.2Kw;额定电压380V;额定电流0.72A;防护等级IP55;绝缘等级F级;安装方式B14;额定转速1350r/min;Y形接法，S3工作制","台","2","2024-12-30","炼钢厂部"]
[2,"A2244000310140","6000200295","绕线式转子电机","YZR160L-6H 11Kw 双轴","JB/T10105-1999 中心高度160 11KW 380V 6极 940r/min绝缘等级H 双轴输出","台","2","2024-12-30","炼钢厂部"]
[3,"A2246000390014","6000201204","高效率三相异步电动机","YE4-100L2-4;3KW；带小齿轮","额定电压 380V; 额定电流 6.5A; 额定转速 1430r/min ;绝缘等级F; 防护等级IP55 ; 安装方式B5 ;接线方式 Y;功率因素0.82;50HZ;出厂编号16201","台","1","2024-12-30","炼钢厂部"]
[4,"A2246000700219","6000200677","变频调速三相异步电动机","YVF2-90S-4;1.1Kw","额定电压380V;额定电流2.7A;额定转速1400r/min;绝缘等级F; 防护等级IP55; 接线方式:Y形","台","1","2024-12-30","180热轧"]
[5,"A2247000270213","6000200834","异步交流电动机","YEZ132S-6;4Kw","电流11A，转速930R/min 电压380V IP44 B5","台","1","2024-12-30","炼铁厂部"]
[6,"A2247000270214","6000200829","异步交流电动机","YEZ112S-4;3Kw","电流7.6A，转速1380R/min 电压380V IP44 B5","台","1","2024-12-30","炼铁厂部"]
[7,"A2247000270215","6000200830","异步交流电动机","YEZ112L-4;4.5Kw","电流10.5A，转速1380R/min 电压380V 50HZ IP44 B5","台","1","2024-12-30","炼铁厂部"]
[8,"A2247000440012","6000201117","交流异步电动机","BPYXKK630-8W","功率2800Kw;额定电压6000V;额定电流334.1A;额定频率50Hz;绝缘等级F级;防护等级IP54;转速740r/min;S1工作制;Y型接法;冷却方式IC616","台","1","2024-12-30","炼钢厂部"]
[9,"A2247000440013","6000200699","变频三相异步电动机","YSP315L-4","B3 185Kw 336A;;恒功率范围50－67HZ IP54 F级 接法 三角型","台","1","2024-12-30","炼钢厂部"]
[10,"A2248000830244","6000201267","变频电动机","YP2 400L2-6MT2","额定功率315KW，额定电流590A，变频范围：1-100HZ，防护等级IP54,三角形接法，994r/min,工作制S1，绝缘等级F","台","1","2024-12-30","180热轧"]
[11,"A2249000350049","6000200233","交流电动机","YA802-4 0.75Kw","额定功率：0.75KW,额定电流：1.6A，转速：1390RPM，效率0.71，功率因素：0.75，安装方式：B3","台","1","2024-12-30","炼钢厂部"]
[12,"A2249000390001","6000200378","锥型转子电动机","ZD32-4 4.5Kw 3T电动葫芦用","JB/T5330-2007 额定功率4.5KW 4极 额定转速1380r/min","台","1","2024-12-30","炼钢厂部"]
[13,"A2249000590049","6000201283","三相异步电动机","DM180/BM/HF/TF/V","功率：22KW;46A;380V;额定转速:1470rpm;防护等级:IP55;频率:3-50-100HZ;安装方式：B5；出厂编号：1100020489/1-001;厂家:宁波东力","台","1","2024-12-30","340热轧"]
[14,"A2249000590079","6000201283","三相异步电动机","DM180/BM/HF/TF/V","功率：22KW;46A;380V;额定转速:1470rpm;防护等级:IP55;频率:3-50-100HZ;安装方式：B5；出厂编号：1100020489/1-001;厂家:宁波东力","台","1","2024-12-30","340热轧"]
[15,"A2249000680179","6000201232","三相异步电动机","YE3 160M2-2","额定功率15KW；额定电流27.4A；能效等级3级；额定电压380V；防护等级IP55；噪声83dB（A）；额定频率50HZ；工作制S1；效率93.3%；功率因数0.89；额定转速2930r/min；绝缘F级","台","1","2024-12-30","180热轧"]
[16,"A2249000680268","6000200329","交流电动机","CT03-1HP-4P-3JV","0.75KW 220V/380V 内孔12.7 内孔键槽14.3*3.2","台","4","2024-12-30","180管加工热处理"]
[17,"A224A000280148","6000201082","交流电动机","YE4-132S-4 5.5Kw","380V;绝缘等级F级;IP44;B5;Δ型接线方式;11.6A;1440r/min;电机尾端不带风叶与风罩,尾端轴不伸出尾端盖,不带接线盒，带1m长电机引出线;出轴端钻孔攻丝∮10mm*20mm?前端法兰盘四个孔要带丝∮16mm.","台","1","2024-12-30","炼铁厂部"]
[18,"A224A000280152","6000201153","变频电机","YZP112M-6M","2.2KW，B3,380V,6.0A,变频范围3-100Hz,50Hz,930r/min,IP54,Y型，F绝缘","台","2","2024-12-30","炼铁厂部"]
[19,"A224A000280162","6000200197","交流电动机","Y2EJ-132S-4-MT28/B5 5.5kW","电压:380VAC 绝缘等级:H 防护等级:IP55 安装方式:B5 接线方式:三角型接法 S5工作制","台","2","2024-12-30","炼铁厂部"]
[20,"A1249000360045","6000200956","交流电动机","DM225S-4","额定功率：37KW;额定电压:380V;额定电流:70A;防护等级:IP55;频率:50HZ;额定转速:1480rpm;出厂编号1100043635/4-1;厂家:宁波东力","台","1","2024-12-30","89管加工热处理"]
[21,"A1249000360056","6000200119","交流电动机","Y280S-4 75Kw","AC380V F级 IP54 IM B3 接线△ 138A 1480r/min 标准编号 JB/T10391-2008","台","1","2024-12-30","89管加工热处理"]
[]
["注：1、投标报价含税，税率13% ；                                                                                                                \n2、生产厂家要求全称填写准确无误 ；                                                                                                               \n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年11月电动机招标采购项目                      项目编号：HG JY-G2024141"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]