{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":43,"n_cols":14,"rows_kept":43,"merged":[[0,0,0,12],[1,0,1,12],[39,0,39,9],[40,0,40,9],[41,0,41,9],[42,0,42,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年11月电气备件采购项目                 项目编号：HG JY-G2024145"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A1246000350004",6100900158,"变频器柜","MD880-01S-0673-4-SG-CT","含变频器MD880-01S-0673-4-SG；进线断路器NSX800F TMD 800 3P3D F，熔断器HDLRT0-1000+熔芯 800A，制动单元MDBUN-200-T，EtherNet卡HETN-10，柜体GGD 800*2200*600","EN61800-3","套",1,"219厂部","2024-12-27"]
[2,"A1249000360042",6200200654,"伺服控制器","IS580T100-R1","INPUT 3PH AC380-480V 106A OUTPUT AC 0-480V,112A 0－300HZ 55KW SUZHOU LNOUANCE","JB/T8219-1999","套",1,"89管加工热处理","2024-12-27"]
[3,"A1249000360043",6200300123,"抗干扰六脉冲控制板","KGPS-6D","控制电源AC18V, 频率0-2500HZ ，主回路进线电源AC380V","SJ/T10616-1995","块",2,"89管加工热处理","2024-12-27"]
[4,"A1249000360044",6100600313,"半导体设备保护用熔断器","RSK-500V/800A-07ALK","额定电压500V，电流800A","IEC60269-4","只",5,"89管加工热处理","2024-12-27"]
[5,"A1249000410091",4100500409,"APT带灯旋钮开关","PB1S-11CXD/G23","绿色;AC/DC24V;一开一闭;孔径22.5mm;防护等级IP65","IEC60947-5-1","只",50,"219厂部","2024-12-27"]
[6,"A1249000410104",4100600073,"行车防震高清投影灯","SBLJWB200W","输入电压220V，功率200W LED，色温8000-8500K,防护等级IP65","GB/T28037-2011","台",2,"219厂部","2024-12-27"]
[7,"A124A000510024",6300500289,"工业以太网交换机","IE4320-20P","16个10/100/1000BASE-T电口，4个1000BASE-X SFP端口，交换容量336Gpps,包转发率120Mpps,双路备份冗余输入24~48VDC（18~55VDC），卡轨安装","GB/T9813-2000","台",2,"89管加工热处理","2024-12-27"]
[8,"A2248000450039",6100600101,"快熔","NGTC1","1000V/250A",null,"个",10,"炼钢厂部","2024-12-27"]
[9,"A2248000540065",6100500375,"时间继电器","SSJ-21A","额定电压：DC220v;触头类型：双延时0.02-9.99s即二付独立动合触点，一付瞬时动转换触点;厂家：上海华兴自动化设备厂;","GB 14048.4","只",3,"340热轧","2024-12-27"]
[10,"A2249000170005",6100900161,"防爆电气控制箱","600*800*250；380V；铸铝材质","380V","JB14048.6","台",1,"能源厂部","2024-12-27"]
[11,"A2249000350025",6200200998,"IGBT功率模块","2MBI1400VXB-120P-54","容量1400A;耐压1200V;MYS","GB/T1404","块",1,"炼钢厂部","2024-12-27"]
[12,"A2249000350026",6200200999,"整流模块","MDC500A/1600V","容量5000A;耐压1600V","GB/T18904-2002","块",1,"炼钢厂部","2024-12-27"]
[13,"A2249000350057",7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2024-12-27"]
[14,"A2249000390021",4000200382,"耐磨型集电器组件","PB31DD-NMX2000Z","包含全套精密铸造支架、D66材质合金电刷、铜导线、导电铜托盘、高强度绝缘子组件等;具备清灰功能;可连续使用30天","GB/T6391-2010","套",50,"炼钢厂部","2024-12-27"]
[15,"A2249000390022",4000200383,"耐磨型集电器组件电刷","PB31DD-NM2000-DS","D66材质;沁铜工艺和金电刷;200*80*35等;具备清灰功能;可连续使用30天","GB/T6391-2010","只",50,"炼钢厂部","2024-12-27"]
[16,"A2249000680182",6200200980,"行走变频器","S500-1.5G/2.2P","变频器品牌艾默生，输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流3.8A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-12-27"]
[17,"A2249000680183",6200200981,"滚轮变频器","S500-2.2G/4P","变频器品牌艾默生，输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流5.1A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-12-27"]
[18,"A2249000680184",6200200982,"主电机变频器","S500-G18.5/22P","变频器品牌艾默生输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流37A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-12-27"]
[19,"A2249000680202",6100600312,"熔断器","ATDR6","6A;AC 200KA;IR600V;DC100KA IR300V","GB/T13539 IEC 60270","只",100,"180热轧","2024-12-27"]
[20,"A224A000280140",6200200924,"温湿度采集板","HD90S-C1-THB21",98030416,"GB/T14315-2008","块",1,"炼铁厂部","2024-12-27"]
[21,"A224A000450019",6000201282,"仓壁振动器","CZ600","功率0.15Kw;电压220V;激振力0-6KN;电流2.3A;频率50Hz;振频3000r/min;防护等级IP55;接法Y;绝缘等级F;工作制S1","JB/5330-2007","台",2,"炼钢厂部","2024-12-27"]
[22,"A224A000450021",6400400185,"增量编码器","DFS60B-TEEL00500","TTL增量编码器;DC10-32V;信号通道数量6通道;输出频率≤600kHZ;负载电流≤30mA; 夹紧法兰M12;通孔空心轴;运行温度范围-40℃-100℃;SICK","DIN 2301-1158","个",1,"炼钢厂部","2024-12-27"]
[23,"A224A000450023",6200201013,"高压变频器功率单元","1200G37N","输入电压3相690V/50HZ;输出电压0-690V","DL/T2033-2019","台",1,"炼钢厂部","2024-12-27"]
[24,"A224A000450024",6200100108,"整流桥","MDC-380A/1600V","AC380V*DC1600V*380A","GB50062-1992","块",2,"炼钢厂部","2024-12-27"]
[25,"A224A000450025",6200201014,"IGBT模块","GD450HFY120C2S","IGBT模块GD450HFY120C2S;VCES = 1200V，IC nom = 450A / ICRM = 900A*-20℃～130℃","GB/T20079-2006","块",1,"炼钢厂部","2024-12-27"]
[26,"A224A000450026",6200201015,"IGBT模块","GD600HFY120C6H","IGBT模块GD450HFY120C2S;VCES = 1200V，IC nom = 600A / ICRM = 1200A*-20℃～130℃","GB/T20079-2006","块",1,"炼钢厂部","2024-12-27"]
[27,"A224A000450027",6200201033,"电流互感器","LMZ1-0.5 4000/5A","变比4000/5A;等级0.5;一次穿心;1T","GB1208-2006","个",2,"炼钢厂部","2024-12-12"]
[28,"A224A000450034",4100700172,"声光报警器","TGSG-06A","额定电压380V",null,"台",5,"炼钢厂部","2024-12-27"]
[29,"A1249000090039",4100500039,"行程开关","LX19-111",null,"GB/T14048","只",10,"物流中心","2024-12-27"]
[30,"A124A000460123",6300300159,"ControlNet通信模块","1756-CN2/C","1756-CN2/C","IEC61508","块",4,"219厂部","2025-01-26"]
[31,"A224B000120002",6100100270,"数字式线路保护装置B柜","CSC-103","含线路保护装置CSC-103A-GCN（1台）；      操作箱JFZ-12FX-CN(含电压切换)1台；        光纤复接通道接口装置CSC-186GBN（2台）；打印机LQ-350K-T1P2G0（1台）；           柜体及附件TG1G（1面）；","GB/T25840-2010","台",1,"能源厂部","2025-01-27"]
[32,"A224B000120001",6100100269,"数字式线路保护装置A柜","PCS-931","含线路保护装置PCS-931型1台；          断路器保护装置PCS-923A （1台）；             CZX-120G-H2操作箱（1台）； MUX-2MD复用接口装置（2台）； 打印机1台；  柜体1面（含附件）；","GB/T25840-2010","台",1,"能源厂部","2025-01-27"]
[33,"A224A000580044",6100900189,"变频器成套控制柜","BSC-280/380","柜体尺寸：800（宽）*800（深）*2200（高）；内附：变频器IPE300-0280-4；制动单元DBU100H-320-4；中文面板安装套件IPE300-LCD；DP 总线卡EC-TX503D；断路器CVS600F /600A；接触器CJ20-630J/220V/630A；输入电抗器GDL-ACL0580-4AL 580A；输出电抗器GDL-OCL0660-4AL 660A；铜排60*6","EN61000-6-2","套",1,"180热轧","2024-12-27"]
[34,"A2247000730006",6200200161,"逆变器","20G14NC205JA0NNNNN","110Kw ND 205A 90KW HD 400VAC  FRAME6 配 20-750-2262C-2R和20-HIM-A6","E0.967X","台",2,"720厂部","2025-01-27"]
[35,"A2247000730007",6200200748,"逆变器","20G14NC456JN0NNNNN","250kw（重载200kw），电流456安，直流供电，配20-HIM-A6，20-750-2262C-2R,20-750-PBUS",null,"台",1,"720厂部","2025-01-27"]
[36,"A224B000210182",6000300283,"EOC电机保护器","EOCRSSD-05S","负载电流0.5-6A","GB/T14598.18-2012","个",10,"炼铁厂部","2025-01-27"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年11月电气备件采购项目                 \n项目编号：HG JY-G2024145"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]