{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":25,"n_cols":14,"rows_kept":25,"merged":[[0,0,0,9],[1,0,1,13],[21,0,21,9],[22,0,22,9],[23,0,23,9],[24,0,24,9]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年12月机械备件采购项目                     项目编号：HG JY-G2024161"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A124A000480124",5700800433,"重载直线导轨副","GZB65BALZZ3P12×1720-4-35/35","导轨长1720mm；配三滑块","套",2,"JB/T 12603-2016","89热轧","2025-01-26"]
[2,"A124A000480125",5700800434,"直线导轨滑块","GZB65BALZZP1-4H-R1-A-G","成品","套",4,"JB/T 12603-2016","89热轧","2025-01-26"]
[3,"A2248000480117",7100100287,"高压阀门","HYKY01-ZCL0104","DN20;PN300","只",2,"GB/25376-2010","炼钢厂部","2025-01-26"]
[4,"A2248000800053",7101600281,"高温烟气调节阀","LSQF-1W-G","DN1700;输入信号4-20mADC，输出4-20mADC;阀杆，阀体不锈钢，工作温度0-450℃；质保2年，宗曼（上海）阀门制造有限公司","台",1,"GB/T4213-2008","180管加工热处理","2025-01-26"]
[5,"A2249000350012",6600300146,"雾化调节阀","OKV2107057-6","定位器 TYPE:RAD-RH/POS1 SIZE:400 BENCH SET:0-33 TRAVEL 90DegC PRESS UNITS: PSI  阀体 TYPE:1001 SIZE:3 PORT SIZE:3 RATING:CL150RF PLUG CF3M/CR PL STEM: S20910 BODY:WCC SEAT:S21800","台",1,"ASME","炼钢厂部","2025-01-26"]
[6,"A224B000040001",5712400018,"卧式带锯机","G42100；含电气、液压控制系统及前后两组对中夹紧装置；","含电气、液压控制系统及前后两组对中夹紧装置；","台",1,"GB/16454-2008","炼钢厂部","2025-02-26"]
[7,"A224B000560078",5201500019,"直线导轨（E=30)","HGW35CA2R1900Z0CⅡ","长度1900mm;每根带2个配套导轨滑块","件",4,"GB/T4250","炼钢厂部","2025-01-27"]
[8,"A224B000670042",5300800003,"三相低压36V轨道供电电动平车","KPD-40;","非标","台",1,"JB/T 6127-2010","180热轧","2025-02-11"]
[9,"A224B000740058",5501800036,"气液自动调整恒压清扫器","ZL-ZIIB-HB1000","100毫米宽刮刀，自动上下调整；磨损自动补偿，清扫压力显示，万向扭力张紧器 ；","套",2,"审核图纸","高辅工段","2024-12-28"]
[10,"A224B000560016",5602600075,"事故切割枪","SG-III","弯嘴型;L=2400mm;附订货图QGJ-23","把",6,"GB5108-1985","炼钢厂部","2025-01-27"]
[11,"A224B000560116",5602600076,"单倍尺割枪","LDG-16改","割枪总长1765;枪体1600;切割氧管接口DG1\";预热氧管接口DG3/4\";燃气管路接口DG3/4\"（左）;冷却水管接口DG1/2","把",10,"GB5108-1985","炼钢厂部","2025-01-27"]
[12,"A124B000250001",5900100040,"拉伸机平夹块","TPH106D1.01.10.01-01a","夹持范围：2-50mm，安装方式：燕尾槽+4孔，适合试样尺寸（2～50mm）；用于万测自动100吨拉伸机，一套共4块，上下各左右两块","套",2,"GB/T16826-2008","检验检测中心","2025-01-27"]
[13,"A124B000250002",5900100041,"平行气爪","AF30-90-N0-PS","使用压力：3-7bar，重复精度：0.02mm；用于万测自动100吨拉伸机配套的ABB机器人组件，一套共两片","套",2,"GB/T9872-1999","检验检测中心","2025-01-27"]
[14,"A224B000670120",7101600286,"Bray气动对夹式碟阀","BWHSam-S42-DN150","DN150,阀体WCB，  阀芯316SS ,  气缸S92,   电磁阀S63E，压力等级300#","只",4,"GB/T4213-2008","180热轧","2025-01-27"]
[15,"A224B000560018",7502300081,"气水喷嘴头","PZWH5.1-80-60HY-1","二冷水和压缩空气;板式连接;角度80＊60o;流量5.1L/min;不含底座;附订货图","只",1000,"YB4187-1992","炼钢厂部","2025-01-27"]
[16,"A224B000560117",7502300083,"430活动段喷嘴","HPZ1.0-90QZ2","材质:黄铜;最大喷射角度90度;水流量1.0l/min(2bar)","只",100,"J11Q20961R3M","炼钢厂部","2025-01-27"]
[17,"A224B000680040",7502500126,"冷却塔风机","LF-60IIB;厂家：惠阳航空螺旋桨有限责任公司","转速165r/min;流量1000000m3/h;全压115pa;带桨叶安装装置（包含轮毂、夹具、紧固螺栓等）不带桨叶","台",1,"JB/T2977-1992","180管加工热处理","2025-01-27"]
[18,"A224B000270008",7102100011,"气动控制阀门","D376XE70",null,"只",5,"ISO5211","340管加工热处理","2025-01-27"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年12月机械备件采购项目        项目编号：HG JY-G2024161"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]