{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["清单计价表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"清单计价表","index":0,"n_rows":78,"n_cols":11,"rows_kept":78,"merged":[[0,0,0,8],[1,0,1,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,2,8],[77,0,81,8]],"flags":["formulas_cached_only"]}
["340厂厂房延伸建安工程工程量清单计价表","","","","","","","","","",""]
["工程名称：340厂厂房延伸建安工程 ","","","","","","","",null,"",""]
["序号","项目编码","项 目 名 称","项 目 特 征 描 述","工作内容","计量\r\n单位","工程量","金额(元)","","",""]
["","","","","","","","综合单价","合  价","",""]
["","","一、建筑工程","","",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"",""]
["1","011602001001","混凝土道路/地面破除","1.混凝土道路/地面破除\r\n2.废渣运距:外运出衡钢厂、 弃土场由乙方自理","1.拆除; 2.控制扬尘;\n3.清理; 4.废渣外运;","m3",80,0,0,"",""]
["2","011602002001","钢筋混凝土基础破除","1.钢筋混凝土基础破除;\r\n2.外运废渣钢筋不外露;\r\n3.废渣运距:外运出衡钢厂、 弃土场由乙方自理;","1.拆除; 2.控制扬尘;\n3.清理; 4.废渣外运;","m3",50,0,0,"",""]
["3","01B001","屋面及墙面彩钢瓦保护性拆除","1.屋面及墙面彩钢瓦保护性拆除;\n2.废渣外运出衡钢厂，弃土场由乙方负责;\n3.拆除的彩钢瓦整理堆放到甲方指定地点;","1.拆除、控制扬尘;\r\n2.清理、转运、垃圾外运;","m2",2201,0,0,"",""]
["4","011601001001","砖砌体拆除","1.砖砌体拆除;\n2.废渣运距:外运出衡钢厂、 弃土场由乙方自理","1.拆除; 2.控制扬尘;\n3.清理; 4.废渣外运;","m3",42,0,0,"",""]
["5","011611005001","厂房钢结构保护性拆除","1.构件名称:厂房钢结构保护性拆除;\r\n2.拆除的钢结构堆放到甲方指定地点;","1.拆除; 2.控制扬尘;\r\n3.清理; 4.转运、废渣运输;","t",65,0,0,"",""]
["6","01B002","行车钢轨道保护性拆除","1.行车钢轨道拆除;\r\n2.规格：行车钢轨道QU70;\r\n3.拆除的废钢堆放到甲方指定地点;","1.拆除; 2.控制扬尘;\n3.清理; 4.废渣外运;","m",54,0,0,"",""]
["7","01B003","滑触线（含支架）拆除","1.滑触线（含支架）拆除;\r\n2.规格：60*6角钢;","1.拆除; 2.控制扬尘;\n3.清理; 4.废渣外运;","m",162,0,0,"",""]
["8","010101004001","挖基础土方","1.挖土深度:约2.5m;\r\n2.土壤类别:综合;\r\n3.按《2020年湖南省建筑装饰工程消耗量标准》计算规则计算","1.排地表水;\r\n2.土方开挖;\r\n3.基底钎探;","m3",3200,0,0,"",""]
["9","010103001001","回填方","1.密实度要求:0.93以上;\n2.土石方运输    3.回填                         \n4.分层夯实","1.挖土方  2.装卸、运输\r\n3.回填   4.分层碾压、夯实","m3",2800,0,0,"",""]
["10","010103002001","余方弃置","1.运距:外运出衡钢厂、 弃土场由乙方自理;","1.挖土方及杂物\r\n2.装卸、运输\r\n3.整平","m3",400,0,0,"",""]
["11","010516001001","预埋螺栓","1.螺栓种类:综合;\r\n2.按螺杆、双螺母、单垫片重量计算，螺栓固定架在综合单价中考虑","1.螺栓制作、运输;\r\n2.螺栓安装;","t",8,0,0,"",""]
["12","01B004","植钢筋","1.钢筋直径：Φ16及以上\r\n2.钢筋甲方供应，钢筋价格不计入合同单价","1.定位、钻孔、清孔、植钢筋","根",300,0,0,"",""]
["13","01B005","植钢筋","1.钢筋直径：Φ14及以下\r\n2.钢筋甲方供应，钢筋价格不计入合同单价","1.定位、钻孔、清孔、植钢筋","根",500,0,0,"",""]
["14","01B006","二次灌浆","1.C35细石混凝土;","1.砼制作         2.运输         \n3.浇筑、振捣      4.养护                                  \n5.模板制作、安装、拆除","m3",2,0,0,"",""]
["15","010501001001","垫层","1.混凝土强度等级:C15;\r\n2.厚度:100mm;","1.模板及支撑制作、安装、拆除、堆放、运输及清理模内杂物、刷隔离剂等;\r\n2.混凝土制作、运输、浇筑、振捣、养护;","m3",63,0,0,"",""]
["16","010501003001","独立基础","1.混凝土强度等级:C30;","1.混凝土制作、运输、浇筑、振捣、养护","m3",295,0,0,"",""]
["17","011702001001","独立基础模板","1.基础类型:独立基础;\r\n","1.模板制作;\r\n2.模板安装、拆除、整理堆放及场内外运输;\r\n3.清理模板粘结物及模内杂物、刷隔离剂等;","m2",522,0,0,"",""]
["18","010503001001","基础梁","1.混凝土强度等级:C30;","1.混凝土制作、运输、浇筑、振捣、养护;","m3",45,0,0,"",""]
["19","011702005001","基础梁模板","1.梁截面形状:综合;","1.模板制作;\r\n2.模板安装、拆除、整理堆放及场内外运输;\r\n3.清理模板粘结物及模内杂物、刷隔离剂等;","m2",300,0,0,"",""]
["20","010502001001","柱包脚","1.混凝土强度等级:C25;","1.混凝土制作、运输、浇筑、振捣、养护;","m3",15,0,0,"",""]
["21","011702002001","柱包脚模板","1.柱包脚模板","1.模板制作;\r\n2.模板安装、拆除、整理堆放及场内外运输;\r\n3.清理模板粘结物及模内杂物、刷隔离剂等;","m2",68,0,0,"",""]
["22","010515001001","现浇混凝土钢筋","1.钢筋种类：各种规格   \r\n2.钢筋甲方供应，钢筋价格不计入合同单价","1．钢筋制作、运输、安装                                           2．钢筋固定所需材料不另计算","t",20,0,0,"",""]
["23","010603001001","钢柱","1.钢材品种、规格:主要为组合焊接H型钢;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",100,0,0,"",""]
["24","010604001001","屋面梁","1.钢材品种、规格:主要为焊接H型钢;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",75,0,0,"",""]
["25","010603001002","抗风柱","1.钢材品种、规格:主要为轧制H型钢;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",12,0,0,"",""]
["26","010604002001","行车梁","1.钢材品种、规格:主要为焊接H型钢;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",90,0,0,"",""]
["27","010606001001","柱间支撑","1.钢材品种、规格:综合;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",5,0,0,"",""]
["28","010606001002","钢支撑、钢拉条","1.钢材品种、规格:综合;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作;\r\n2.安装;\r\n3.刷油漆;","t",60,0,0,"",""]
["29","010606007001","钢走道板","1.钢材品种、规格:综合;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",21,0,0,"",""]
["30","010606008001","钢梯、钢栏杆等钢结构","1.钢材品种、规格：Q355-B，综合;\r\n2.除锈等级：Sa2 1/2;\r\n3.油漆品种及漆膜厚度：两底一中两面、环氧富锌底漆、环氧云铁中间漆、聚氨酯面漆，厚度按设计;\r\n4.钢材甲方供应，钢材费不计入综合单价;\r\n5.油漆甲方供应，油漆材料费不计入综合单价;","1.制作、拼装;\r\n2.安装;\r\n3.探伤;\r\n4.刷油漆;","t",10,0,0,"",""]
["31","010606011001","不锈钢天沟","1.钢材品种、规格:2mm厚不锈钢板\r\n2.钢材甲方供应，钢材费不计入综合单价;","1.制作   2.运输\r\n3.安装","t",6,0,0,"",""]
["32","010606002001","屋面檩条","1.钢材品种、规格:采用高强镀锌Z型钢檩条，镀锌量不小于275g/m 强度Q345A  \r\n2.钢材甲方供应，钢材费不计入综合单价","1.制作   2.运输\r\n3.安装   4.刷油漆;","t",50,0,0,"",""]
["33","010606002002","墙面檩条","1.钢材品种、规格:采用高强镀锌C型钢檩条，镀锌量不小于275g/m 强度Q345A  \r\n2.钢材甲方供应，钢材费不计入综合单价","1.制作   2.运输\n3.安装","t",30,0,0,"",""]
["34","010901002001","屋面采光瓦","1.规格：1.5mm厚阻燃型玻璃纤维增强聚酯采光波型板，板形与屋面一致。        \n2.采光板选用宽度为760mm, 采光板抗紫外线要求99%，散射率>90%，玻璃纤维含量>30%，透光率~72%\n3.按水平投影面积计算，包边、包角、搭接含在综合单价内不另计算;","1.制作、运输、安装","m2",545,0,0,"",""]
["35","010605001001","压型钢板屋面","1.压型钢板厚度、规格、品牌:采用蓝色彩色压型钢板厚0.6mmYX51-380-760型,单层隐藏式连接角弛-Ⅲ，热镀锌基板,二涂二烤,彩钢平板厂家为宝武集团钢板宝钢板                    2.按水平投影面积计算，包边、包角、搭接含在综合单价内不另计算","1.制作\n2.运输\n3.安装\n4.接缝、嵌缝","m2",5530,0,0,"",""]
["36","010605002001","压型钢板墙板","1.压型钢板厚度、规格、品牌:采用蓝色彩色压型钢板厚0.5mm，U-820型,单层隐藏式连接角弛-Ⅲ，热镀锌基板,二涂二烤,彩钢平板厂家为宝武集团钢板宝钢板                             2.按垂直投影面积计算，包边、包角、搭接含在综合单价内不另计算","1.制作\n2.运输\n3.安装\n4.接缝、嵌缝","m2",1175,0,0,"",""]
["37","010605002002","墙面采光板","1.规格：1.5mm厚阻燃型玻璃纤维增强聚酯采光波型板，板形与墙面一致。        \n2.采光板选用宽度为760mm, 采光板抗紫外线要求99%，散射率>90%，玻璃纤维含量>30%，透光率~72%\n3.按垂直投影面积计算，包边、包角、搭接含在综合单价内不另计算","1.制作、运输、安装","m2",1100,0,0,"",""]
["38","010803001001","金属卷帘门","1.门材质:1.2mm厚铝合金;\r\n2.启动装置品种、规格:电动;","1.门运输、安装\n2.启动装置、活动小门、五金安装","m2",135,0,0,"",""]
["39","030105001001","行车轨道","1.安装部位:钢吊车梁;\r\n2.固定方式:压条固定法;\r\n3.接头:热铝焊接头（焊接联接）;\r\n4.型号:QU70;\r\n5.计算规则:按轨道延长米长度计算，车挡不另计;\r\n6.钢轨甲方供应，钢轨材料费不计入综合单价;","1.轨道安装;\r\n2.接头制安;\r\n3.车挡制作、安装;","m",450,0,0,"",""]
["40","010807001001","铝合金组合窗（推拉窗＋中翻窗）","1.框、扇材质:80系列;\r\n2.玻璃品种、厚度:5mm平板玻璃;\r\n3.其他:含制作、安装、窗锁、五金、窗套等全部工作内容;","1.窗安装;\r\n2.五金、玻璃安装;","m2",186,0,0,"",""]
["41","010401003001","实心砖墙","1.砖的品种规格及强度等级:MU10 标准页岩砖;\r\n2.墙体厚度:240;\r\n3.砂浆强度等级、配合比:混合MU5.0;   ","1.砂浆制作、运输\n2.砌砖、刮缝、砖压顶砌筑\n3.脚手架搭拆、材料运输","m3",77,0,0,"",""]
["42","011201001001","外墙水泥砂浆抹灰","1.面层厚度：20mm;　\n2.砂浆配合比：1：2;","1.基层清理            \n2.抹面层            \n3.材料运输","m2",290,0,0,"",""]
["43","011201001002","内墙水泥砂浆抹灰","1.面层厚度：20mm;　\n2.砂浆配合比：1：2;","1.基层清理;\r\n2.砂浆制作、运输;\r\n3.抹灰;","m2",210,0,0,"",""]
["44","011406001001","外墙面墙漆","1.刮腻子遍数: 两遍;\r\n2.油漆品种、刷漆遍数: 外墙漆 三遍;","1.基层清理\n2.刮腻子\n3.刷、喷外墙漆","m2",290,0,0,"",""]
["45","011407001001","内墙乳胶漆","1.刮腻子要求:见设计;\r\n2.刷内墙乳胶漆","1.基层清理\n2.刮腻子\n3.刷、喷内墙漆","m2",210,0,0,"",""]
["46","010507001001","散水","1.面层厚度:100厚C20混凝土 面加5mm厚1:1水泥砂浆随捣随抹;\r\n2.详见设计;","1.地基夯实   \n2.混凝土制作、运输、浇筑、振捣、养护\n3.变形缝填塞","m2",145,0,0,"",""]
["47","010401014001","砖砌明沟","1.砖品种、规格、强度等级:片岩砖;\r\n2.沟截面尺寸:平均深度约300mm;\r\n3.垫层材料种类、厚度:C15;\r\n4.具体见设计;","1.土方挖、运、填;\r\n2.铺设垫层;   3.砌砖;\r\n4.刮缝、抹灰; 5.材料运输;","m",185,0,0,"",""]
["","","二、安装部分","","",{"v":0,"d":"0.00"},0,0,0,"",""]
[48,"030404017002","动力配电箱","1.规格型号:见设计;\r\n2.安装方式:挂墙式;\r\n3.配电箱甲方供货、配电箱材料费不计入综合单价;\r\n4.基础槽钢/支架角钢甲方提供，材料费不计入综合单价;","1.支架制作、安装 2.箱体安装、调试","台",1,0,0,"",""]
[49,"030404017001","照明配电箱(含检修箱、应急配电箱）","1.规格型号:见设计;\r\n2.安装方式:挂墙式;\r\n3.检修箱甲方供货、配电箱材料费不计入综合单价;\r\n4.基础槽钢/支架角钢甲方提供，材料费不计入综合单价;","1.支架制作、安装 2.箱体安装、调试","台",6,0,0,"",""]
[50,"030404017003","吊车电源开关箱","1.名称:吊车电源开关箱;\r\n2.安装方式:挂墙式;\r\n3.型号:见设计;\r\n4.开关箱甲方供货、开关箱材料费不计入综合单价;\r\n5.基础槽钢/支架角钢甲方提供，材料费不计入综合单价;","1.支架制作、安装 2.箱体安装、调试","台",3,0,0,"",""]
[51,"030409008001","等电位端子箱","1.规格型号:按设计;\r\n2.安装方式:按设计;\r\n3.端子箱甲方供货、端子箱材料费不计入综合单价;","1.本体安装;","台",1,0,0,"",""]
[52,"030411003001","电缆桥架及附件 b=600","1.槽式/梯级式电缆桥架、600（宽）*100mm\r\n2.按桥架延长米长度计算\r\n3.桥架及附件(如:连接片、调高片、螺栓等）甲方供货，不计入综合单价","1.本体安装、附件安装;","m",230,0,0,"",""]
[53,"031002001001","桥架支撑架","1.托臂、立柱(镀锌)\r\n2.桥架支撑架甲方供货、桥架支撑架费不计入综合单价","1.安装;\r\n2.补刷油漆;","t",4.5,0,0,"",""]
[54,"030412002001","LED工矿灯","1.LED工矿灯;\r\n2.安装位置：屋架下弦;\r\n3.灯具甲方提供、灯具费不计入综合单价;","1.本体安装、接线、支架/吊杆制作安装；","套",100,0,0,"",""]
[55,"030407001001","滑触线","1.规格:L63*6 角钢滑触线;\r\n2.滑触线甲方提供、滑触线材料费不计入综合单价;","1.滑触线安装;\r\n2.滑触线支架制作、安装;\r\n3.拉紧装置及挂式支持器制作、安装;\r\n4.伸缩接头制作、安装;","m",675,0,0,"",""]
[56,"030411001001","电气配管 G20","1.镀锌钢管  G20\r\n2.按管道延长米长度计算，各种附件不另计价\r\n3.管道甲方供货、主材费不计入综合单价","1．管道敷设        2．接地、跨接","m",300,0,0,"",""]
[57,"030411001003","电气配管 G50","1.镀锌钢管  G50\r\n2.按管道延长米长度计算，各种附件不另计价\r\n3.管道甲方供货、主材费不计入综合单价","1．管道敷设        2．接地、跨接","m",60,0,0,"",""]
[58,"030408001001","电力电缆","1.三芯及以上电缆、 单芯截面10mm2以下（含10mm2）\r\n2.按电缆延长米长度计算，附件不另计价\r\n3.电缆甲方供货、电缆主材费不计入综合单价","1.电缆敷设、固定 2.接线 \n3.试验 4.防火堵洞、电缆防护","m",2360,0,0,"",""]
[59,"030408006001","低压电力电缆头","1.型号:三芯及以上电缆、 单芯截面10mm2以下（含10mm2）\r\n2.电缆头及铜鼻子等附件乙方提供","1.电力电缆头制作;\r\n2.电力电缆头安装;\r\n3.接地;","个",200,0,0,"",""]
[60,"030409002001","接地母线 -40*4","1.接地母线 镀锌扁钢-40*4\r\n2.按扁钢延长米长度计算，附件不另计价\r\n3.扁钢甲方供货、扁钢材料费不计入综合单价","1.接地母线敷设","m",400,0,0,"",""]
[61,"03B001","虹吸雨水口","1.虹吸雨水斗YG100A\r\n2.材质：304不锈钢","1.制作、运输、安装;","个",30,0,0,"",""]
[62,"031001006001","HDPE塑料排水管","1.管道规格：φ110*4.2mm;\r\n2.连接方式：热熔;","1.管道、管件安装;\r\n2.固定管卡安装;\r\n3.压力试验、吹扫、冲洗;\r\n4.灌水试验;","m",145,0,0,"",""]
[63,"031001006002","HDPE塑料排水管","1.管道规格：φ160*6.2mm;\r\n2.连接方式：热熔;","1.管道、管件安装;\r\n2.固定管卡安装;\r\n3.压力试验、吹扫、冲洗;\r\n4.灌水试验;","m",140,0,0,"",""]
[64,"031001006003","HDPE塑料排水管","1.管道规格：φ200*7.7mm;\r\n2.连接方式：热熔;","1.管道、管件安装;\r\n2.固定管卡安装;\r\n3.压力试验、吹扫、冲洗;\r\n4.灌水试验;","m",80,0,0,"",""]
[65,"031001006004","HDPE塑料排水管","1.管道规格：φ250*9.6mm;\r\n2.连接方式：热熔;","1.管道、管件安装;\r\n2.固定管卡安装;\r\n3.压力试验、吹扫、冲洗;\r\n4.灌水试验;","m",5,0,0,"",""]
[66,"031001006005","HDPE塑料排水管","1.管道规格：φ315*12.1mm;\r\n2.连接方式：热熔;","1.管道、管件安装;\r\n2.固定管卡安装;\r\n3.压力试验、吹扫、冲洗;\r\n4.灌水试验;","m",60,0,0,"",""]
[67,"031002001002","零星钢支架制安","1.材质:Q235B;\r\n2.支架种类:管道吊架等;\r\n3.油漆:除锈后刷防锈漆二道,再刷调和面漆二道;\r\n4.钢材甲方供应，钢材费不计入综合单价\r\n5.油漆甲方提供、油漆材料费不计入综合单价","1.制作;\r\n2.安装;\r\n3.油漆","t",2.5,0,0,"",""]
[null,null,"三、其他"]
[68,"01B007","绿色施工安全防护措施费",null,null,"项",1,null,0]
[69,"01B008","暂列金额","1.目前未预见到、在实施过程中有可能会发生的其他零星项目;","1.此项按甲方提供金额报价，不得修改;","项",1,100000,100000]
[{"$nulls":3},"合    计"]
["清单报价说明：1、综合单价为不含税价，开票税率 %（增值税）。\n                       2、除注明设备/材料甲方（业主）供外，其余均由施工单位供应，发包方供应的材料和设备均由承包方自行到发包方仓库(或甲方指定地点)领取，领用和运输所需\n                的费用应包含在各自的投标报价中。\n                       3、混凝土等级调差：C30以下（含C30）每个等级差为：10元/m3，C30以上每个等级差为：15元/m3\n                       4、电力电缆敷设中列出三芯及以上，如为二芯/单芯电缆则按《2020年湖南省安装工程消耗量标准》计算规则执行"]