{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":26,"n_cols":14,"rows_kept":26,"merged":[[0,0,0,9],[1,0,1,13],[22,0,22,9],[23,0,23,9],[24,0,24,9],[25,0,25,9]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2025年1月机械备件采购项目                项目编号：HG JY-G2025007"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A124B000250002",5900100041,"平行气爪","AF30-90-N0-PS","使用压力：3-7bar，重复精度：0.02mm；用于万测自动100吨拉伸机配套的ABB机器人组件，一套共两片","套",2,"GB/T9872-1999","检验检测中心","2025-03-28"]
[2,"A124C000360130",5400300045,"低氮天然气高速烧嘴","SFSV180(250)N-380T","烧嘴前压力大于3.5kpa.","套",3,"GB/T26800-2011","219厂部","2025-03-28"]
[3,"A124C000360131",5400300046,"低氮天然气高速烧嘴","SFSV600N-380T","烧嘴前压力大于3.5kpa.","套",3,"GB/T26800-2011","219厂部","2025-03-28"]
[4,"A124C000360132",7102600103,"燃气电磁阀","SG40/32RQ/220","电源：220AC","件",6,"GT/T7223-1994","219厂部","2025-03-28"]
[5,"A124C000360133",7102600104,"燃气电磁阀","SG25RQ/220","电源：220AC","件",6,"GT/T7223-1994","219厂部","2025-03-28"]
[6,"A124C000360136",6600300206,"电动执行器+蝶阀","SAM4P+HTB125S(H)","电源：220AC,±10%，50HZ,逻辑输入：220AC,±10%，50HZ，电流5mA,电流反馈：4-20mA,精度1%","套",4,"TB/T8219-1999","219厂部","2025-03-28"]
[7,"A124C000360137",6600300207,"电动执行器+蝶阀","SAM4P+HTB65S(H)","电源：220AC，±10%，50HZ，逻辑输入：220AC，±10%，50HZ，电流：5mA，电流反馈：4-20mA，精度1%","套",4,"TB/T8219-1999","219厂部","2025-03-28"]
[8,"A2248000800053",7101600281,"高温烟气调节阀","LSQF-1W-G","DN1700;输入信号4-20mADC，输出4-20mADC;阀杆，阀体不锈钢，工作温度0-450℃；质保2年，宗曼（上海）阀门制造有限公司","台",1,"GB/T4213-2008","180管加工热处理","2025-03-28"]
[9,"A224B000270008",7102100011,"气动控制阀门","D376XE70",null,"只",5,"ISO5211","340管加工热处理","2025-03-28"]
[10,"A224B000560116",5602600076,"单倍尺割枪","LDG-16改","割枪总长1765;枪体1600;切割氧管接口DG1\";预热氧管接口DG3/4\";燃气管路接口DG3/4\"（左）;冷却水管接口DG1/2","把",10,"GB5108-1985","炼钢厂部","2025-03-28"]
[11,"A224B000670042",5300800003,"三相低压36V轨道供电电动平车","KPD-40;","非标","台",1,"JB/T 6127-2010","180热轧","2025-03-28"]
[12,"A224C000030001",5601700015,"四流喂丝机","WFIV-A","额定功率9.3*4KW;额定电压380V;额定频率50/60HZ;速度0-6m/s;PLC控制;变频器调速;尺寸1860*960*2450mm","台",1,"GB/T12668","炼钢厂部","2025-03-28"]
[13,"A224C000030002",7001500007,"罗茨真空泵","ER30000","流量30000m3/h;重量2200Kg;No18211003","台",1,"Q/SOEU17-2007","炼钢厂部","2025-03-28"]
[14,"A224C000030009",6100100126,"补偿器","LGD-YN-72000","2000V/72000A;电流密度2.6;最大电阻48u欧","只",3,"Q320282PEQ001-2011","炼钢厂部","2025-03-28"]
[15,"A224C000160023",7501600004,"加药罐装置","PT-3000L","3m3，PE材质，配计量泵一台（耐腐蚀泵，500l/h，0.5MPa），配搅拌装置（304不锈钢搅拌杆和叶轮，1.1kw），PPR阀门及水管一批","套",2,"GB4806-2016","能源厂部","2025-03-28"]
[16,"A224C000340115",5501200134,"柔性翻板式新型双层卸灰装置","JYXF300×1800","\"驱动方式：下阀板分别由单个独立液压缸驱动；液压站（含滤油器+缓冲装置）：电机功率：2.2KW   厂家：节能高效电机\n油泵：康百世齿轮泵   ；密封件材质：橡胶软密封（耐温200℃）；工作压力：16Kpa～20Kpa；物料堆重比：2.2t/m3；漏风率：≤0.05%\"","套",4,"审核图纸","烧结","2025-03-28"]
[17,"A224C000700123",7502300074,"喷嘴","1/4PZ48-65-QZ5","连接螺纹1/4;全水喷嘴;喷水面形状为圆形;最大流量7L/MIN(0.7MPa）;最小流量1.2L/MIN(0.1MPa）;附订货图XHY0223J0-GBS3102.6-4-10","只",500,"JB/T12492-2015","炼钢厂部","2025-03-28"]
[18,"A224C000750001",7001500003,"罗茨真空泵","DDR40000（2030144）","极限压力0.03Pa;抽速40000m3/h;转速Max3600r/min;功率37Kw;带电机","台",1,"Q/SOEU17-2007","炼钢厂部","2025-03-28"]
[19,"A224A000280020",5500100015,"上密封阀阀座","直径700mm","Cr64Mo 高铬合金钢，Cr64Mo，调质处理，铬含量64‰，含成套高强度螺栓及氟橡胶密封件","件",1,null,"高炉","2025-03-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2025年1月机械备件采购项目       项目编号：HG JY-G2025007"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]