{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":8,"n_cols":13,"rows_kept":8,"merged":[[0,0,0,8],[1,0,1,12],[4,0,4,8],[5,0,5,8],[6,0,6,8],[7,0,7,8]],"flags":["formulas_cached_only"]}
[]
["项目名称：炼钢厂废钢场白灰场移位改造新建除尘器采购项目                       项目编号：HGJSG2025011"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,null,"滤筒","φ160×3000","单个滤筒过滤面积≤6.90m2、滤筒材质：ePTFE覆膜聚酯针刺毡，滤筒有效使用寿命≥36个月，颗粒物排放满足≤10mg/Nm³，滤筒绑带间距差异小于0.5mm；滤筒折数≤46，折深≤25mm，滤筒要求一体成型。滤筒透气量满足（EN ISO 9237）标准要求，滤筒耐温120℃。折叠滤筒满足《袋式除尘用折式滤筒技术要求》（T/CAEPI 72-2023）要求。","条",800,"T/CAEPI 72-2023","炼钢厂","2024-04-20",null,null,"白灰场新建除尘器包安装"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}