{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":11,"rows_kept":9,"flags":["formulas_cached_only"]}
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期"]
[1,"A1252000430011",5900100048,"卧式带锯床","430B","锯切能力：圆料：?430 mm；方料：430W X 430Hmm；方料：410W X 195Hmm；控制方式：PLC+触摸屏+按钮；进给方式：液压(智能变速)；工作夹紧方式：液压虎钳；排屑方式：液压螺旋排屑机；带锯条张紧方式：液压","台",1,"JB/T4318.3——2013","检验检测中心","2025-05-29"]
[2,"A2252000800080",6200201047,"高压变频器功率单元","HD90S-J100/450-DN","\"单元型号：HD9MS-A069-0030-40000A，尺寸:515*380*275 ,重量：4.7KG    \n电压690V/30A，两电平两象限功率单元(不含单元旁路功能)；厂家：汇川\"","套",2,"GB/T12668.4-2006","180热轧","2025-05-29"]
[3,"A2251000210093",6100900012,"端子盒","1.314014","端子盒 长宽高312*403*141","只",2,"JB/T10634-2006","340热轧","2025-05-29"]
[4,"A1251000490002",6700400301,"60吨电子拉伸（液压平推）试验机","600kN","试验机级别0.5级；额定功率7kW；平推液压夹具(带油源)","套",1,"GB/T 228.1","检验检测中心","2025-05-29"]
[5,"A1251000490003",6700400302,"高温拉伸试验机","300KN","微机控制电子万能试验机；配高低温箱+高温炉+全自动引伸计","套",1,"GB/T 228.2","检验检测中心","2025-05-29"]
[6,"A1251000490004",6700400303,"弯曲试验机","500kN","三缸弯曲试验机；最大垂直推力500kN；最大水平推力400kN","套",1,"GB/T 232-2010","检验检测中心","2025-05-29"]
[7,"A2253000390001",9400500005,"风动送样系统","MLF-RT-A","发送站MLF-RT-A-1，1台，接收站MLF-RT-A-2，1台，泄压装置FDSY-09-02，2套；开盖装置MLF-ZD-00，2套；送样盒MLF-ZDYH，5个；\n送样直管精轧冷拔无缝钢管650米；送样弯管精轧冷拔无缝钢管18根；数据传输系统MLF-TERM,1套;PLC电控系统PLC S7-200smart,1套;\n光电传感器装置2套;储气罐1m3，2个。","套",1,null,"炼钢分厂","2025-05-29"]
[8,"A2252000130001",7101300026,"气动执行器","B1CU25/95L","双作用；最大压力：1.0Mpa；温度范围：-55-120℃；品牌：NELES","台",3,"ISO5211","能源厂部","2025-05-29"]