{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":16,"rows_kept":6,"merged":[[1,0,4,0],[1,10,4,10]],"flags":["formulas_cached_only"]}
["标包","序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","备注","申请部门","交货期","含税单价（元）","含税金额（元）","生产厂家","备注"]
[1,1,"G2250300280002","B200100151","风冷冷风型空调机","LF22N，    \n Q冷=21.7kW， 配电功率：N=8kW/380V ","侧出风，前回风。面对空调机，左配管5台，室内机与室外机距离各16米，配室外机各1台，带气管、液管，带风帽。电源由室内组接入，空调电源开关均设置在室内机侧","台",5,"包安装","HG202321： 一炼钢5#机开坯机一炼钢",4.19]
[null,2,"G2250300280006","B200100155","风冷冷风型空调机","LF86N\nQ冷=85.6kW，配电功率：N=35kW/380V","顶出风，前回风。面对空调机，左配管3台，室内机与室外机距离各18米，配室外机各3台，带气管、液管，带风帽。电源由室内组接入，空调电源开关均设置在室内机侧。","台",3,"包安装",null,4.19]
[null,3,"G2250300280007","B200100156","风冷冷风型空调机","LF43N\nQ冷=42.5kW， 配电功率：N=18kW/380V ","侧出风，前回风。面对空调机，左配管1台，右配管1台，室内机与室外机距离各15米，配室外机各2台，带气管、液管，带风帽。电源由室内组接入，空调电源开关均设置在室内机侧。","台",2,"包安装",null,4.19]
[null,4,"G2250300280015","B200100164","风冷冷风型空调机","LF33N  Q冷=32.7kW， 配电功率：N=12.55kW/380V  ","侧出风，前回风。面对空调机，右配管1台，室内机与室外机距离6米，配室外机1台，带气液管，带风帽。电源由室内组接入，空调电源开关均设置在室内机侧","台",1,"包安装",null,4.19]
[{"$nulls":4},"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}