{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":28,"n_cols":14,"rows_kept":28,"merged":[[0,0,0,9],[1,0,1,13],[24,0,24,9],[25,0,25,9],[26,0,26,9],[27,0,27,9]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年7月机械备件采购项目                     项目编号：HG JY-G2024097"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2246000760108",5712800023,"鼓风机","D680-12；右旋90°（含风机、轴承箱带水冷及电机）","全压12000Pa；流量9200-40000Nm3/h；转速1450r/min；电机型号YPT355M-4；功率200kW","台",1,"JB/T10563-2006","720厂部","2024-09-26"]
[2,"A2246000760004",6600300199,"氧气自力式调压阀","ZZYP-16PB","压力6Mpa，通径：DN80，阀前压力1.5-1.6Mpa，阀后压力0.1-0.2Mpa，介质为氧气，配法兰及紧固件。","件",1,"GB/T 12244-2006","720厂部","2024-08-27"]
[3,"A1246000270001",6700400291,"液压压紧化验制样粉碎机","GJE200-3","一次制样3个，装料粒度小于20毫米；装料重量每钵200克；粉碎时间小于3分钟；出料粒度120-200目；外形尺寸1200*900*1000；重量220kg；1.5Kw","台",1,null,"物流中心","2024-09-11"]
[4,"A1246000270002",6700400292,"液压压紧化验制样粉碎机","GJE500-1","一次制样1个，装料粒度小于26毫米；装料重量每钵500克；粉碎时间小于3分钟；出料粒度120-200目；外形尺寸1200*900*1000；重量250kg；1.5Kw","台",1,null,"物流中心","2024-09-11"]
[5,"A2246000660071",7100100285,"气动调节阀","HPTYS-16K  DN150 PN16 CV640","阀体材质316，阀座316L，附件：西门子定位器隔爆，减压阀，手轮机构，法兰及紧固件硬密封，上阀盖标准型，温度-20～450℃，输入输出信号：4-20mA，介质氧气，脱脂禁油，泄漏等级六级，流量特性：等百分比，高精度阀芯","套",2,"JB/T 450-2008","340管加工热处理","2024-08-27"]
[6,"A2246000700207",7102600099,"离心式气源干燥器","AF-03","工作介质：压缩空气；流量2.0/Min；工作压力0.3-1.6Mpa；","台",5,"GB/T13927-1994","180热轧","2024-07-28"]
[7,"A2246000760006",7102600102,"气动薄膜调节阀","YSIQ-10-25K-BKD,DN100","阀门DN100,阀体材质304不锈钢，流体介质为氧气，使用温度-40℃--150℃；配不锈钢法兰与紧固件。","台",1,"GB/T4213-1993","720厂部","2024-08-27"]
[8,"A2246000530011",7502300067,"气水喷嘴","PZWH5.1-80-60HY","二冷水和压缩空气;板式连接;角度80*60o;流量5.1L/min","只",300,"YB4187-1992","炼钢厂部","2024-08-12"]
[9,"A1245000450091",7001200350,"除磷环喷嘴紫铜垫","MQL-CLH-01","材质：紫铜；重量：0.02kg","只",100,"审核图纸","89管加工热处理","2024-08-26"]
[10,"A2244000540107",5800100035,"压缩弹簧","d=22;D=210;H0=900;有效圈数10;两段并紧磨平","65Si2MnA","根",2,"GB/T1972-1992","720厂部","2024-08-26"]
[11,"A2244000600191",5704900004,"内磨机磨杆","M52型","长度6.9m,直径52mm,内轴20mm,80kg","根",2,"JB/T3715-2016","180热轧","2024-08-26"]
[12,"A2246000160087",7501300140,"金属补偿器","CCHFCG-1002","上法兰450*400/下法兰410*410， 加内衬；重量20.6kg","件",10,"审核图纸","高辅工段","2024-08-12"]
[13,"A2246000160118",7102600100,"气动梭阀","DN25 PN16 CF8 DVC200 0.3-0.8MPa",null,"只",4,"GB/T4213-2008","烧结","2024-07-28"]
[14,"A2246000160121",5300400311,"压带轮装置","80Y11",null,"套",1,"GB10595-2009","烧结","2024-07-28"]
[15,"A2246000160122",5300400312,"压带轮装置","100Y11",null,"套",1,"GB10595-2009","烧结","2024-07-28"]
[16,"A2246000160123",5300400313,"压带轮装置","65Y11",null,"套",1,"GB10595-2009","烧结","2024-07-28"]
[17,"A2246000160205",5501800036,"气液自动调整恒压清扫器","ZL-ZIIB-HB1000","100毫米宽刮刀，自动上下调整；磨损自动补偿，清扫压力显示，万向扭力张紧器 ；","套",8,"审核图纸","原料工段","2024-07-28"]
[18,"A2246000160206",5501800037,"气液自动调整恒压清扫器","ZL-ZIIB-HB800","100毫米宽刮刀，自动上下调整；磨损自动补偿，清扫压力显示，万向扭力张紧器;","套",4,"审核图纸","原料工段","2024-07-28"]
[19,"A2246000220080",5705300022,"带锯机","G4250/85",null,"台",2,"JB/T4318.4-2002","180热轧","2024-09-11"]
[20,"A2244000310290",7102000081,"燃气止回阀","HF-G1A","内丝G1\";球头;介质:氧气","只",5,"GB13347-1992","炼钢厂部","2024-08-26"]
[21,"A2245000180103",5501200112,"烧结机点火炉烧嘴","HX-5a","天然气内芯、煤气内芯不锈钢","套",9,"审核图纸","烧结","2024-08-26"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年7月机械备件采购项目        项目编号：HG JY-G2024097"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]