{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":23,"n_cols":14,"rows_kept":23,"merged":[[0,0,0,13],[1,0,1,13],[19,0,19,9],[20,0,20,9],[21,0,21,9],[22,0,22,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年8月电磁备件采购项目                     项目编号：HG JY-G2024108"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2247000440016",4100400039,"电缆卷筒","DF100/20-45/35-8/8","容量100A 8通道 电缆长度20米","台",1,"JT/T806.4-2011","炼钢厂部","2024-11-10"]
[2,"A2247000440040",4100400047,"电缆卷筒弹簧","JTA100-25-2-Ⅱ","JTA100-25-2-Ⅱ型电缆卷筒用弹簧","只",10,"JT/T806.4-2011","炼钢厂部","2024-11-10"]
[3,"A2247000490041",4100400052,"电缆连接器","DL-202","快速接头容量200A双通道","只",5,"GB/T19446-2004","炼钢厂部","2024-11-10"]
[4,"A2247000440017",4100400298,"电缆快速连接头","KMDL-60/80w","额定电流;500A","套",24,"GB/T19446-2004","炼钢厂部","2024-09-26"]
[5,"A2247000450016",6000300125,"气管卷筒","QJDF-50F/20","带力矩电机及减速机","台",1,"JT/T806.4-2011","炼钢厂部","2024-10-11"]
[6,"A1245000450034",4100400052,"电缆连接器","DL-202","快速接头容量200A双通道","只",2,"GB/T19446-2004","89管加工热处理","2024-09-10"]
[7,"A1245000460014",4100400051,"电缆卷筒专用碳刷","JTA100-20-2","JTA100-20-2型电缆卷筒用专用碳刷","付",10,"DL-478","219厂部","2024-09-10"]
[8,"A1246000210048",5300600117,"电缆卷筒弹簧","1.6*40*22000","直径340mm，单层厚度1.6mm，宽度40mm，长度22m，合金弹簧钢","个",1,"Q/0100 ANY006—2019 GB/T 1222-2016","检验检测中心","2024-09-10"]
[9,"A2245000720133",6000400010,"永磁吸吊器","YX1-0.3",null,"台",1,"CB/T3555-1994","720厂部","2024-09-10"]
[10,"A2246000530107",6000400010,"永磁吸吊器","YX1-0.3",null,"台",1,"CB/T3555-1994","炼钢厂部","2024-09-11"]
[11,"A1246000120025",6100900059,"无触点停电保持柜","LMOBM-200/20-C-UPS-T","进线AC380，输出直流电压DC220V,采用恒电流控制，输出电流可调,最大220A，停电保持时间20MIN，控制器S7-200,电器元件为Schneider","台",1,"JB/T8680-2008","物流中心","2024-09-26"]
[12,"A2244000430071",6100100097,"整流控制柜变压器","ZSG-30KVA/170+190","GB/T18494.1-2001 30KVA 输入380V 输出170+190V","台",1,"JB4315-1986","340热轧","2024-09-10"]
[13,"A1245000080006",6100500432,"电磁吸盘电压检测板","FV1-FV2","输入电压DC170V-260V","套",1,"IEC97-1991","物流中心","2024-09-10"]
[14,"A1246000310001",6200100104,"电磁吸盘主控电路板","CFB-2X6K-AC220V","输入电压AC220V，输出电压DC221V","块",1,"GB/T3235-1999","物流中心","2024-09-10"]
[15,"A1246000310002",6200100105,"电磁吸盘充电电路板","CFB-1X6K-DC220V","输入电压AC14V+14V+8V，输出电压DC220V","块",1,"GB/T3235-1999","物流中心","2024-09-10"]
[16,"A2245000470038",4100400307,"电动气管卷筒","LT0400F-0-1","卷取长度30m;力矩120N;带力矩电机及减速机","台",2,"JT/T806.4-2011","炼钢厂部","2024-09-10"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年8月电磁备件采购项目        项目编号：HG JY-G2024108 "]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}