{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["开标一览表","偏离表"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"开标一览表","index":0,"n_rows":11,"n_cols":14,"rows_kept":11,"merged":[[0,0,0,9],[1,0,1,13],[7,0,7,5],[8,0,8,6],[9,0,9,6],[10,0,10,6]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：二炼钢大包烘烤位等功能区移位拆迁工程项目 (HG202256)工业空调一批采购项目             项目编号：HG JS-G2024078"]
["序号","物料描述","规格型号","技术参数","计量单位","定尺尺寸\n其他要求","计划数量","执行标准","建议交货日期","供货地点","含税单价\n（元）","含税合价（元）","生产厂家","备注   "]
[1,"风冷冷风型空调机","LF43N","QL=42.5kW N=16.14kW/380V","台","带风帽，面对出风口\n右侧配管1台，左侧配管1台\n气管、液管分别总长30m",2,"GB/T1527-2006","2023.10.15","江依人计划；3#电炉操作室空调"]
[2,"分体立柜式冷暖空调机","KFR-120L/MSD","QL=12kW QR=16.5kW N=8.2kW/380V","台",null,5,"GB/T1527-2006","2023.10.15","江依人计划；3#电炉操作室空调"]
[3,"风冷冷风型空调机","LF21N","QL=20.8kW N=7.88kW/380V","台","带风帽，面对出风口\n左侧配管1台\n气管、液管分别长7m\n",1,"GB/T1527-2006","2023.10.15","江依人计划；3#电炉操作室空调"]
[{"$nulls":5},"总价"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"偏离表","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：二炼钢大包烘烤位等功能区移位拆迁工程项目 (HG202256)工业空调一批采购项目             项目编号：HG JS-G2024078"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]