{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["一、开标一览表","二、商务 技术偏离"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一、开标一览表","index":0,"n_rows":88,"n_cols":11,"rows_kept":88,"merged":[[0,0,0,10],[1,0,1,5],[1,6,1,10],[85,0,85,10],[86,0,86,10],[87,0,87,10]],"flags":["formulas_cached_only"]}
["开  标  一  览  表"]
["项目名称：2024年11月-2025年11月五金日杂年标采购项目   ",{"$nulls":5}," 项目编号：HG JY-G2024135"]
["序号","物料编码","物料描述","规格描述","技术参数","单位","年需求数量","交货日期","含税单价（元）","生产厂家","备注"]
[1,"3300600037","铁屑","1mm≤粒度≤4mm","要求干燥、无油","吨",10,"以订单为准",null,null,"实际需求量以订单为准"]
[2,"3301000010","工业盐NaCL","(细)",null,"吨",60,"以订单为准",null,null,"实际需求量以订单为准"]
[3,"3301000023","洗洁精","2.5kg/瓶",null,"瓶",150,"以订单为准",null,null,"实际需求量以订单为准"]
[4,"3400100019","彩条布","8m宽",null,"米",1800,"以订单为准",null,null,"实际需求量以订单为准"]
[5,"3400100042","白钢玉砂轮片","(φ350*φ127*40)mm","100目","片",150,"以订单为准",null,null,"实际需求量以订单为准"]
[6,"3400100054","小砂带","10*330mm","1200目","根",690,"以订单为准",null,null,"实际需求量以订单为准"]
[7,"3400100058","棉纱","10kG",null,"Kg",7800,"以订单为准",null,null,"实际需求量以订单为准"]
[8,"3400100059","棉布","10kG",null,"Kg",4600,"以订单为准",null,null,"实际需求量以订单为准"]
[9,"3400300008","冰块","420*560*180",null,"块",1100,"以订单为准",null,null,"实际需求量以订单为准"]
[10,3301000071,"工业盐NaCl(粗)","粗盐","颗粒盐、粗盐","吨",50,"以订单为准",null,null,"实际需求量以订单为准"]
[11,"4000200094","尼龙扎带","4*200mm",null,"根",46200,"以订单为准",null,null,"实际需求量以订单为准"]
[12,"4000200095","尼龙扎带","5*300mm",null,"根",32500,"以订单为准",null,null,"实际需求量以订单为准"]
[13,"4000200096","尼龙扎带","6*400mm",null,"根",40800,"以订单为准",null,null,"实际需求量以订单为准"]
[14,"4000200098","尼龙扎带","GT-150",null,"根",8400,"以订单为准",null,null,"实际需求量以订单为准"]
[15,"4000300031","毛刷","75-80mm",null,"把",630,"以订单为准",null,null,"实际需求量以订单为准"]
[16,"4000300032","毛刷","100mm",null,"把",530,"以订单为准",null,null,"实际需求量以订单为准"]
[17,"4000300077","钢丝绳用铝套管","A型;","直径14mm","只",8000,"以订单为准",null,null,"实际需求量以订单为准"]
[18,"4000400004","白色粉笔","*",null,"盒",4400,"以订单为准",null,null,"实际需求量以订单为准"]
[19,"4000400005","白色油性笔","CNSSA10",null,"支",6500,"以订单为准",null,null,"实际需求量以订单为准"]
[20,"4000400027","记号笔","兰/黑",null,"支",350,"以订单为准",null,null,"实际需求量以订单为准"]
[21,"4000400070","可赛新超兰","TM1587,","310ml/支","支",600,"以订单为准",null,null,"实际需求量以订单为准"]
[22,"4000400074","松动剂","1750型","500ml","瓶",200,"以订单为准",null,null,"实际需求量以订单为准"]
[23,"4000400082","电池7#","*",null,"对",240,"以订单为准",null,null,"实际需求量以订单为准"]
[24,"4000400112","螺纹锁固密封胶","277","250ml/支","支",80,"以订单为准",null,null,"实际需求量以订单为准"]
[25,"4000400116","石英光棒","长16mm，直径3.8mm",null,"根",3000,"以订单为准",null,null,"实际需求量以订单为准"]
[26,"4000400120","平板拖把","*","60cm","把",70,"以订单为准",null,null,"实际需求量以订单为准"]
[27,"4000400123","绝缘橡皮垫","800mm*5mm",null,"Kg",2700,"以订单为准",null,null,"实际需求量以订单为准"]
[28,"4000600006","斗车","手推式",null,"辆",80,"以订单为准",null,null,"实际需求量以订单为准"]
[29,"4000600040","货运电动三轮车","电池6020;带盒",null,"组",30,"以订单为准",null,null,"实际需求量以订单为准"]
[30,"4000600044","303单动式矮型千斤顶","JRSM-502；","50吨","台",20,"以订单为准",null,null,"实际需求量以订单为准"]
[31,"4000700006","布拖把","*",null,"把",2000,"以订单为准",null,null,"实际需求量以订单为准"]
[32,"4000700014","灰斗","*",null,"只",120,"以订单为准",null,null,"实际需求量以订单为准"]
[33,"4000700017","芦苇扫把","*",null,"把",2000,"以订单为准",null,null,"实际需求量以订单为准"]
[34,"4000700029","有柄铁铲","2#(长柄1.5M)",null,"把",2000,"以订单为准",null,null,"实际需求量以订单为准"]
[35,"4000700030","竹扫把","*",null,"把",420,"以订单为准",null,null,"实际需求量以订单为准"]
[36,"4000700031","棕扫把","*",null,"把",1500,"以订单为准",null,null,"实际需求量以订单为准"]
[37,"4100400025","包塑金属软管","φ32mm(电气专用)",null,"米",500,"以订单为准",null,null,"实际需求量以订单为准"]
[38,"4100900013","角磨机切割片","直径100mm*1.2mm*直径16mm DIN",null,"片",1200,"以订单为准",null,null,"实际需求量以订单为准"]
[39,"4100900014","砂带","200*1630mm","200*1630mm 粒度 60","张",1500,"以订单为准",null,null,"实际需求量以订单为准"]
[40,"4100900015","砂带","XK870*P36","4000*150mm","根",1300,"以订单为准",null,null,"实际需求量以订单为准"]
[41,"4100900025","芯棒焊条","Castolin 6 F2248","NHSS*3.2mm","Kg",250,"以订单为准",null,null,"实际需求量以订单为准"]
[42,"4100900026","园柱磨头","直径25*30","直径25*30","只",1500,"以订单为准",null,null,"实际需求量以订单为准"]
[43,"4100900032","弹力精磨片","*","125mm","块",25000,"以订单为准",null,null,"实际需求量以订单为准"]
[44,"4100900039","树脂磨片","SBD-STA4502A-125","125mm","片",57600,"以订单为准",null,null,"实际需求量以订单为准"]
[45,"4100900043","硬布砂带","LD4000*150","80目；缝口搭接","条",200,"以订单为准",null,null,"实际需求量以订单为准"]
[46,"4200200007","电动扳手","6906",null,"台",24,"以订单为准",null,null,"实际需求量以订单为准"]
[47,"4200200053","气动冲击扳手","3228—2000",null,"件",12,"以订单为准",null,null,"实际需求量以订单为准"]
[48,"4200700035","模具电磨","SIJ-6 480W",null,"台",80,"以订单为准",null,null,"实际需求量以订单为准"]
[49,"4200700054","移动式检修电缆盘","30米3*2.5+1*1.5","防护等级：IP65#","只",20,"以订单为准",null,null,"实际需求量以订单为准"]
[50,"4200700055","硬质合金开孔器","订货号：630130225 DIN","直径22.5 PG22 DIN EN 60745-2-1-2011","个",15,"以订单为准",null,null,"实际需求量以订单为准"]
[51,"4200700088","充电式角向磨光机","DGA402SFJ/RME/Z  100mm(4'') (18V, 带电池，带充电器）","能力：钹形砂轮片100mm(4'') 回转数（rpm) 10,000 体积（长*宽*高）317*118*118mm ；一次充电工作量：切割混凝土（深度5mm）;15m 左右，切割钢筋10mm：25个左右","台",20,"以订单为准",null,null,"实际需求量以订单为准"]
[52,"4200800035","毛刷","150mm","150mm","把",1800,"以订单为准",null,null,"实际需求量以订单为准"]
[53,"4200900107","可赛新1750松动剂","可赛新1750松动剂,350g/瓶",null,"个",95,"以订单为准",null,null,"实际需求量以订单为准"]
[54,"4201500004","电焊钳","500A",null,"把",100,"以订单为准",null,null,"实际需求量以订单为准"]
[55,"4201700011","附柄砂布轮.","附柄砂布轮80#",null,"个",2400,"以订单为准",null,null,"实际需求量以订单为准"]
[56,"4201700017","角磨片","125*6*22；NO:1669161256",null,"片",5700,"以订单为准",null,null,"实际需求量以订单为准"]
[57,4000200374,"PVC电工胶带",1976,"0.19mm*16.5mm*φ74mm","卷",10000,"以订单为准",null,null,"实际需求量以订单为准"]
[58,"4201700125","角磨片","100*6*16mm","T27   A/F24","片",4000,"以订单为准",null,null,"实际需求量以订单为准"]
[59,"4300100030","超强力万能胶","*","1.6Kg/桶","桶",150,"以订单为准",null,null,"实际需求量以订单为准"]
[60,"4300200009","精密电子仪器清洗剂","780","350g/瓶","瓶",240,"以订单为准",null,null,"实际需求量以订单为准"]
[61,"4300300001","氧气管","10*2*30",null,"根",80,"以订单为准",null,null,"实际需求量以订单为准"]
[62,"4300300003","乙炔管","10*1*30",null,"根",50,"以订单为准",null,null,"实际需求量以订单为准"]
[63,"4300600007","包塑金属软管","φ20mm(电气专用)",null,"米",1200,"以订单为准",null,null,"实际需求量以订单为准"]
[64,"4300600008","包塑金属软管","φ25mm(电气专用)",null,"米",700,"以订单为准",null,null,"实际需求量以订单为准"]
[65,"4500100014","气压管","25*5*20",null,"根",80,"以订单为准",null,null,"实际需求量以订单为准"]
[66,"5300800001","正三轮电动车","车身尺寸：2800*1020*1260箱体尺寸：1300*1020*260","功率800w,车速≤20km/h;载重150kg；把式","台",24,"以订单为准",null,null,"实际需求量以订单为准"]
[67,"6400500785","硅胶板","硅胶板：6mm,硬度40；白色","硅胶板：6mm,硬度40；白色","公斤",500,"以订单为准",null,null,"实际需求量以订单为准"]
[68,"6600200624","Graphite Crucible（石墨坩埚）","775-892(100个/盒)","LECO公司ON736型氧氮分析仪专用石墨坩埚","盒",25,"以订单为准",null,null,"实际需求量以订单为准"]
[69,"7300600017","塑料气管","159666 PUN-8*1.25-BL FESTO",null,"米",1000,"以订单为准",null,null,"实际需求量以订单为准"]
[70,"7300600018","塑料气管","159668 PUN-10*1.5-BL FESTO",null,"米",1500,"以订单为准",null,null,"实际需求量以订单为准"]
[71,"7300600019","塑料气管","159672 PUN-16*2.5-BL FESTO",null,"米",850,"以订单为准",null,null,"实际需求量以订单为准"]
[72,"7300600020","塑料气管","159670 PUN-12*2-BL FESTO","DIN43614-2-1980","米",1300,"以订单为准",null,null,"实际需求量以订单为准"]
[73,"4300600031","塑料气管","159664 PUN-6*1-B","PUN-6*1-BL,FESTO，DN6，厚1","米",600,"以订单为准",null,null,"实际需求量以订单为准"]
[74,7502600012,"风镐","TF-G11","冲击能：45/JSMAX;冲击频率16Hz；缸内径：38mm；行程155mm；耗气量：26L/S;工作气压：0.8-1MPa；使用气管内径19mm","件",50,"以订单为准",null,null,"实际需求量以订单为准"]
[75,"7502600001","风镐","G10",null,"件",80,"以订单为准",null,null,"实际需求量以订单为准"]
[76,"7502900067","手动液压推车","B108.CBY1 2t","1 2t","台",15,"以订单为准",null,null,"实际需求量以订单为准"]
[77,6700100104,"X荧光光谱仪专用分析试剂","X荧光光谱仪专用分析试剂 67Li2B4O7：33LiBO2 有效期内，带有效证书，无水解，无结块变质AR1000g","张家港火炬分析仪器厂","瓶",100,"以订单为准",null,null,"实际需求量以订单为准"]
[78,4200700029,"角向磨光机","GWS6-125","GWS6-125","台",400,"以订单为准",null,null,"实际需求量以订单为准"]
[79,4200700028,"角向磨光机","GWS6-100",null,"台",150,"以订单为准",null,null,"实际需求量以订单为准"]
[80,4400400044,"稀土丝","直径2.1mm","主要元素:铈(Ce)99.98、镧（La）65.79","Kg",280,"以订单为准",null,null,"实际需求量以订单为准"]
[81,4201700130,"砂威125角磨片","125mm*6mm*22.23mm","27-A/F24R8BF；砂威角磨片，最大转速15300r/min 品牌：武汉砂威磨料磨具","件",50000,"以订单为准",null,null,"实际需求量以订单为准"]
[82,4201700138,"砂威100角磨片","100mm*6mm*16mm","27-A/F24R8BF；砂威角磨片，最大转速15300r/min 品牌：武汉砂威磨料磨具","块",15000,"以订单为准",null,null,"实际需求量以订单为准"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：（盖单位章）"]
["法定代表人或其委托代理人：（签字或盖章）"]

{"sheet":"二、商务 技术偏离","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[1,4,1,5],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年11月-2025年11月五金日杂年标采购项目     项目编号：HG JY-G2024135"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]