{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":2,"n_cols":14,"rows_kept":2,"flags":["formulas_cached_only"]}
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A1251000410002","6700400300","全自动冲击试验机","规格：最大冲击能量750J","摆锤冲击试验机带机器人、视觉识别系统、双工位低温箱、电气连接系统、试验软件","套",1,"GB/T 229-2007","检验检测中心","2025-06-30",null,null,"推荐品牌：深圳万测试验设备有限公司（WANCE）、美特斯（MTS）、兹韦克（Zwick）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}