{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","一、开标一览表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":8,"n_cols":14,"rows_kept":8,"merged":[[0,0,0,13],[4,0,4,9],[5,0,5,9],[6,0,6,9],[7,0,7,9]],"flags":["formulas_cached_only"]}
["项目名称：2025年4月应力环支架及气路竞价采购项目                                                               项目编号：HGJYG2025023"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A1251000230036","5900100036","应力环支架及气路","JC20240812-01","长1700mm、宽500mm、高100mm亚克力材质,板材厚8mm；板上8根防滑条、8根加强条；配连接气路，供气管316L材质，供气软管TEFLON材质，三通切换阀型号SS-42GX4材质316，流量调节阀型号SS-ORS2-A材质316，阀组操作面板材质316L，厚1mm；见图纸JC20240812-01。","套","16","检验检测中心","检验检测中心","2025-06-25"]
[2,"A1252000270044","5900100036","应力环支架及气路","JC20240812-01","长1700mm、宽500mm、高100mm亚克力材质,板材厚8mm；板上8根防滑条、8根加强条；配连接气路，供气管316L材质，供气软管TEFLON材质，三通切换阀型号SS-42GX4材质316，流量调节阀型号SS-ORS2-A材质316，阀组操作面板材质316L，厚1mm；见图纸JC20240812-01。","套","16","检验检测中心","检验检测中心","2025-06-25"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]